# EVPN

## nv show evpn

Shows global EVPN control plane information.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show evpn
    perational   applied
    ---------------------  ------------  -------------
    enable                               on
    route-advertise
      nexthop-setting                    system-ip-mac
      svi-ip               off           off
      default-gateway      off           off
    dad
      enable               on            on
      mac-move-threshold   5             5
      move-window          180           180
      duplicate-action     warning-only  warning-only
    [vni]
    multihoming
      enable                             off
      mac-holdtime         1080
      neighbor-holdtime    1080
      startup-delay        180
      startup-delay-timer  --:--:--
      uplink-count         0
      uplink-active        0
    l2vni-count            3
    l3vni-count            2

## nv show evpn access-vlan-info

Shows access VLAN information.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn access-vlan-info
            operational  applied  pending
    ------  -----------  -------  -------
    [vlan]  10
    [vlan]  20
    [vlan]  30
    [vlan]  220
    [vlan]  297
    [vlan]  1000
    [vlan]  3000

## nv show evpn access-vlan-info vlan

Shows all EVPN access VLANs.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn access-vlan-info vlan
    Vlan-id  member-interface-count  vni   vni-count  vxlan-interface  Summary
    -------  ----------------------  ----  ---------  ---------------  -----------------------
    10       1                       10    1          vxlan48          member-interface: bond1
    20       1                       20    1          vxlan48          member-interface: bond2
    30       1                       30    1          vxlan48          member-interface: bond3
    220                                    1          vxlan99
    297                                    1          vxlan99
    1000                             1000  1          vxlan48
    3000                             3000  1          vxlan48

## nv show evpn access-vlan-info vlan <vlan-id>

Shows EVPN access VLAN information for the specified VLAN.

### Command Syntax

Syntax | Description
--- | ---
`<vlan-id>` | The VLAN name.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn access-vlan-info vlan 10
                            operational  applied  pending
    ----------------------  -----------  -------  -------
    member-interface-count  1
    vni                     10
    vni-count               1
    vxlan-interface         vxlan48

    member-interface
    ===================

        -----
        bond1

## nv show evpn access-vlan-info vlan <vlan-id> member-interface

Shows EVPN access VLAN member interface information.

### Command Syntax

Syntax | Description
--- | ---
`<vlan-id>` | The VLAN name.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn access-vlan-info vlan 10 member-interface

    -----
    bond1

## nv show evpn dad

Shows EVPN duplicate address detection information. The VTEP considers a host MAC or IP address to be duplicate if the address moves across the network more than a certain number of times within a certain number of seconds. In addition to legitimate host or VM mobility scenarios, address movement can occur when you configure IP addresses incorrectly on a host or when packet looping occurs in the network due to faulty configuration or behavior.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show evpn dad
                        operational   applied       pending
    ------------------  ------------  ------------  ------------
    enable              off           on            on
    mac-move-threshold  5             5             5
    move-window         180           180           180
    duplicate-action    warning-only  warning-only  warning-only

## nv show evpn dad duplicate-action

Shows the action to take when there is a duplicate address detected.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show evpn dad duplicate-action
     operational   applied       pending
      ------------  ------------  ------------
      warning-only  warning-only  warning-only

## nv show evpn dad duplicate-action freeze

Shows all EVPN duplicate address freeze actions.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show evpn dad duplicate-action freeze
              operational  applied
    --------  -----------  -------
    duration  1000         1000

## nv show evpn l2-nhg

Shows EVPN next hop groups.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn l2-nhg

    vtep-ip
    ==========
        Vtepip      es-ref-count  nexthop-group
        ----------  ------------  -------------
        10.10.10.2  3             268435460
        10.10.10.3  1             268435462
        10.10.10.4  1             268435463

## nv show evpn l2-nhg vtep-ip

Shows EVPN next hop group information for all VTEPs.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn l2-nhg vtep-ip
    Vtepip      es-ref-count  nexthop-group
    ----------  ------------  -------------
    10.10.10.2  3             268435460
    10.10.10.3  1             268435462
    10.10.10.4  1             268435463

## nv show evpn l2-nhg vtep-ip <vtep-id>

Shows EVPN next hop group information for the specified VTEP.

### Command Syntax

Syntax | Description
--- | ---
`<vtep-id>` | The VTEP ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn l2-nhg vtep-ip 10.10.10.2
                   operational  applied  pending
    -------------  -----------  -------  -------
    es-ref-count   3
    nexthop-group  268435460

## nv show evpn multihoming

Shows global EVPM multihoming configuration.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show evpn multihoming
                         operational  applied  pending
    -------------------  -----------  -------  -------
    enable                            on       on
    mac-holdtime         1080         1080     1080
    neighbor-holdtime    1080         1080     1080
    startup-delay        180          180      180
    ead-evi-route
      rx                              on       on
      tx                              on       on
    segment
      df-preference                   32767    32767
    startup-delay-timer  --:--:--
    uplink-active        2
    uplink-count         2

## nv show evpn multihoming bgp-info

Shows EVPN multihoming BGP information.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn multihoming bgp-info
          operational                    applied  pending
    -----  -----------------------------  -------  -------
    [esi]  03:44:38:39:be:ef:aa:00:00:01
    [esi]  03:44:38:39:be:ef:aa:00:00:02
    [esi]  03:44:38:39:be:ef:aa:00:00:03
    [esi]  03:44:38:39:be:ef:bb:00:00:01
    [esi]  03:44:38:39:be:ef:bb:00:00:02
    [esi]  03:44:38:39:be:ef:bb:00:00:03

## nv show evpn multihoming bgp-info esi

Shows EVPN multihoming BGP information for all ESIs.

Add `-o json` at the end of the command to see the output in a more readable format.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn multihoming bgp-info esi -o json
    {
      "03:44:38:39:be:ef:aa:00:00:01": {
        "es-df-preference": 50000,
        "flags": {
          "advertise-evi": "on",
          "up": "on"
        },
        "fragments": {
          "10.10.10.1:3": {
            "evi-count": 1
          }
        },
        "inconsistent-vni-count": 0,
        "macip-global-path-count": 8,
        "macip-path-count": 4,
        "originator-ip": "10.0.0.1",
        "rd": "10.10.10.1:3",
        "remote-vtep": {
          "10.10.10.2": {
            "df-algorithm": "preference",
            "df-preference": 50000,
            "flags": {
              "active": "on",
              "esr": "on"
            }
          }
        },
        "type": {
          "local": "on",
          "remote": "on"
        },
        "vni-count": 1,
        "vrf-count": 1
      },
      "03:44:38:39:be:ef:aa:00:00:02": {
        "es-df-preference": 50000,
        "flags": {
          "advertise-evi": "on",
          "up": "on"
        },
        "fragments": {
          "10.10.10.1:8": {
            "evi-count": 1
          }
        },
        "inconsistent-vni-count": 0,
        "macip-global-path-count": 4,
        "macip-path-count": 2,
        "originator-ip": "10.0.0.1",
        "rd": "10.10.10.1:8",
        "remote-vtep": {
          "10.10.10.2": {
            "df-algorithm": "preference",
            "df-preference": 50000,
            "flags": {
              "active": "on",
              "esr": "on"
            }
          }
        },
    ...

## nv show evpn multihoming bgp-info esi <esi-id>

Shows EVPN multihoming BGP information for the specified ESI.

### Command Syntax

Syntax | Description
--- | ---
`<esi-id>` | The ESI identifier.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn multihoming bgp-info esi 03:44:38:39:be:ef:aa:00:00:02
                             operational   applied  pending
    -----------------------  ------------  -------  -------
    es-df-preference         50000
    inconsistent-vni-count   0
    macip-global-path-count  4
    macip-path-count         2
    originator-ip            10.0.0.1
    rd                       10.10.10.1:8
    vni-count                1
    vrf-count                1
    flags
      advertise-evi          on
      up                     on
    [fragments]              10.10.10.1:8
    [remote-vtep]            10.10.10.2
    type
      local                  on
      remote                 on

## nv show evpn multihoming bgp-info esi <esi-id> remote-vtep

Shows EVPN multihoming BGP information for the specified ESI for all VTEPs.

### Command Syntax

Syntax | Description
--- | ---
`<esi-id>` | The ESI identifier.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn multihoming bgp-info esi 03:44:38:39:be:ef:aa:00:00:02 remote-vtep
                df-algorithm  df-preference  flags.active  flags.esr
    ----------  ------------  -------------  ------------  ---------
    10.10.10.2  preference    50000          on            on

## nv show evpn multihoming bgp-info esi <esi-id> remote-vtep <ipv4-address-id>

Shows EVPN multihoming BGP information for the specified ESI for a specific VTEP.

### Command Syntax

Syntax | Description
--- | ---
`<esi-id>` | The ESI identifier.
`<ipv4-address-id>` | The IPv4 address of the VTEP.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn multihoming bgp-info esi 03:44:38:39:be:ef:aa:00:00:02 remote-vtep 10.10.10.2
                   operational  applied  pending
    -------------  -----------  -------  -------
    df-algorithm   preference
    df-preference  50000
    flags
      active       on
      esr          on

## nv show evpn multihoming bgp-info esi <esi-id> fragments

Shows EVPN multihoming BGP remote VTEP fragment information for a specific ESI.

### Command Syntax

Syntax | Description
--- | ---
`<esi-id>` | The ESI identifier.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn multihoming bgp-info esi 03:44:38:39:be:ef:aa:00:00:02 fragments
                  evi-count
    ------------  ---------
    10.10.10.1:8  1

## nv show evpn multihoming bgp-info esi <esi-id> fragments <fragment-id>

Shows specific EVPN multihoming BGP remote VTEP fragment information for a specific ESI.

### Command Syntax

Syntax | Description
--- | ---
`<esi-id>` | The ESI identifier.
`<fragment-id>` | The route-distinguisher.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn multihoming bgp-info esi 03:44:38:39:be:ef:aa:00:00:02 fragments 10.10.10.1:8
               operational  applied  pending
    ---------  -----------  -------  -------
    evi-count  1

## nv show evpn multihoming ead-evi-route

Shows EVPN multihoming Ethernet Auto-discovery per EVPN instance route information.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show evpn multihoming ead-evi-route
        operational  applied  pending
    --  -----------  -------  -------
    rx               on       on
    tx               on       on

## nv show evpn multihoming esi

Shows EVPN multihoming Ethernet segment ID information.

In Cumulus Linux 5.3 and earlier, this command is `nv show evpn evi`

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn multihoming esi -o json
    {
      "03:44:38:39:be:ef:aa:00:00:01": {
        "df-preference": 50000,
        "flags": {
          "bridge-port": "on",
          "local": "on",
          "nexthop-group-active": "on",
          "oper-up": "on",
          "ready-for-bgp": "on",
          "remote": "on"
        },
        "local-interface": "bond1",
        "mac-count": 2,
        "nexthop-group-id": 536870913,
        "remote-vtep": {
          "10.10.10.2": {
            "df-algorithm": "preference",
            "df-preference": 50000,
            "nexthop-group-id": 268435460
          }
        },
        "vni-count": 1
      },
      "03:44:38:39:be:ef:aa:00:00:02": {
        "df-preference": 50000,
        "flags": {
          "bridge-port": "on",
          "local": "on",
          "nexthop-group-active": "on",
          "oper-up": "on",
          "ready-for-bgp": "on",
          "remote": "on"
        },
        "local-interface": "bond2",
        "mac-count": 2,
        "nexthop-group-id": 536870914,
        "remote-vtep": {
          "10.10.10.2": {
            "df-algorithm": "preference",
            "df-preference": 50000,
            "nexthop-group-id": 268435460
          }
        },
        "vni-count": 1
      },
    ...

## nv show evpn multihoming esi <esi-id>

Shows information about the specified EVPN multihoming Ethernet segment ID.

### Command Syntax

Syntax | Description
--- | ---
`<esi-id>` | The ESI identifier.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn multihoming esi 03:44:38:39:be:ef:aa:00:00:02
                            operational  applied  pending
    ----------------------  -----------  -------  -------
    df-preference           50000
    local-interface         bond2
    mac-count               2
    nexthop-group-id        536870914
    vni-count               1
    flags
      bridge-port           on
      local                 on
      nexthop-group-active  on
      oper-up               on
      ready-for-bgp         on
      remote                on
    [remote-vtep]           10.10.10.2

## nv show evpn multihoming esi <esi-id> remote-vtep

Shows information about the specified EVPN multihoming Ethernet segment ID for remote VTEPs.

### Command Syntax

Syntax | Description
--- | ---
`<esi-id>` | The ESI identifier.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn multihoming esi 03:44:38:39:be:ef:aa:00:00:02 remote-vtep
                df-algorithm  df-preference  nexthop-group-id
    ----------  ------------  -------------  ----------------
    10.10.10.2  preference    50000          268435460

## nv show evpn multihoming esi <esi-id> remote-vtep <ipv4-address-id>

Shows information about a specific EVPN multihoming Ethernet segment ID for the specified remote VTEP.

### Command Syntax

Syntax | Description
--- | ---
`<esi-id>` | The ESI identifier.
`<ipv4-address-id>` | The IPv4 address.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn multihoming esi 03:44:38:39:be:ef:aa:00:00:02 remote-vtep 10.10.10.2
                      operational  applied  pending
    ----------------  -----------  -------  -------
    df-algorithm      preference
    df-preference     50000
    nexthop-group-id  268435460

## nv show evpn multihoming segment

Shows EVPN multihoming segment information.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show evpn multihoming segment
                   operational  applied  pending
    -------------  -----------  -------  -------
    df-preference               32767    32767

## nv show evpn route-advertise

Shows EVPN route advertise information.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show evpn route-advertise
                     operational  applied        pending
    ---------------  -----------  -------------  -------------
    default-gateway  off          off            off
    nexthop-setting               system-ip-mac  system-ip-mac
    svi-ip           off          off            off

## nv show evpn vni

Shows information about the EVPN VNIs on the switch.

In Cumulus Linux 5.3 and earlier, this command is `nv show evpn evi`

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni

    NumMacs - Number of MACs (local and remote) known for this VNI, NumArps - Number
    of ARPs (IPv4 and IPv6, local and remote) known for this VNI
    , NumRemVteps - Number of Remote Vteps

    VNI   NumMacs  NumArps  NumRemVteps  TenantVrf
    ----  -------  -------  -----------  ---------
    10    8        4        3            RED
    20    6        1        3            RED
    30    6        1        3            BLUE
    1000  0        0        0            default
    3000  0        0        0            default

## nv show evpn vni <vni-id>

Shows configuration information about the specified VNI.

In Cumulus Linux 5.3 and earlier, this command is `nv show evpn evi <vni-id>`

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10
                       operational  applied  pending
    -----------------  -----------  -------  -------
    route-advertise
      default-gateway  off
      svi-ip           off
    bridge-domain      br_default
    host-count         4
    local-vtep         10.0.0.1
    mac-count          8
    remote-vtep-count  3
    tenant-vrf         RED
    vlan               10
    vxlan-interface    vxlan48

    remote-vtep
    ==============
                    flood
        ----------  -----
        10.10.10.2  HER
        10.10.10.3  HER
        10.10.10.4  HER

## nv show evpn vni <vni-id> bgp-info

Shows BGP configuration information for the specific VNI.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 bgp-info
                              operational   applied  pending
    -------------------------  ------------  -------  -------
    advertise-default-gateway  off
    advertise-svi-ip           off
    in-kernel                  on
    local-vtep                 10.0.0.1
    rd                         10.10.10.1:5
    type                       L2
    [export-route-target]      65101:10
    [import-route-target]      65101:10

## nv show evpn vni <vni-id> host

Shows the ARP and ND table for the specific VNI.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 host

    LocMobSeq - local mobility sequence, RemMobSeq - remote mobility sequence, Esi -
    Remote Esi

    IP address                 Type    State   LocMobSeq  RemMobSeq  Mac                Esi
    -------------------------  ------  ------  ---------  ---------  -----------------  -------------------------…
    10.1.10.101                local   active  0          0          48:b0:2d:bc:2e:e7
    10.1.10.104                remote  active  0          0          48:b0:2d:d0:1e:4a  03:44:38:39:be:ef:bb:00:0…
    fe80::4ab0:2dff:febc:2ee7  local   active  0          0          48:b0:2d:bc:2e:e7
    fe80::4ab0:2dff:fed0:1e4a  remote  active  0          0          48:b0:2d:d0:1e:4a  03:44:38:39:be:ef:bb:00:0…

## nv show evpn vni <vni-id> host <ip-address-id>

Shows a specific ARP and ND table for the specific VNI.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.
`<ip-address-id>` | The IP address.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 host 10.1.10.101
                         operational        applied  pending
    -------------------  -----------------  -------  -------
    detection-count      0
    duplicate            off
    local-mobility-seq   0
    remote-mobility-seq  0
    type                 local
    mac                  48:b0:2d:bc:2e:e7
    state                active

## nv show evpn vni <vni-id> mac

Shows the MAC address for the specified EVPN VNI.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 mac

    LocMobSeq - local mobility sequence, RemMobSeq - remote mobility sequence,
    RemoteVtep - Remote Vtep address, Esi - Remote Esi

    MAC address        Type    State  LocMobSeq  RemMobSeq  Interface  RemoteVtep  Esi
    -----------------  ------  -----  ---------  ---------  ---------  ----------  -----------------------------
    44:38:39:22:01:7a  local          0          0          vlan10
    44:38:39:22:01:8a  remote         0          0                     10.10.10.4
    44:38:39:22:01:78  remote         0          0                     10.10.10.2
    44:38:39:22:01:84  remote         0          0                     10.10.10.3
    48:b0:2d:1b:21:0e  remote         0          0                                 03:44:38:39:be:ef:bb:00:00:01
    48:b0:2d:91:ee:88  local          0          0          bond1
    48:b0:2d:bc:2e:e7  local          0          0          bond1
    48:b0:2d:d0:1e:4a  remote         0          0                                 03:44:38:39:be:ef:bb:00:00:01

## nv show evpn vni <vni-id> mac <mac-address>

Shows configuration information about a specific VNI MAC address.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.
`<mac-address>` | The MAC address.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 mac 44:38:39:22:01:78
                         operational  applied  pending
    -------------------  -----------  -------  -------
    detection-count      0
    duplicate            off
    local-mobility-seq   0
    remote-mobility-seq  0
    remote-vtep          10.10.10.2
    type                 remote
    neigh-sync-count     0

## nv show evpn vni <vni-id> multihoming

Shows multihoming Ethernet configuration for the specified VNI.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 multihoming
              operational                    applied  pending
    --------  -----------------------------  -------  -------
    bgp-info
      [esi]   03:44:38:39:be:ef:aa:00:00:01
      [esi]   03:44:38:39:be:ef:bb:00:00:01
    [esi]     03:44:38:39:be:ef:aa:00:00:01

## nv show evpn vni <vni-id> multihoming bgp-info esi

Shows BGP information for the multihoming Ethernet segments for the specified VNI.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 multihoming bgp-info esi
                                   type.local  type.remote  Summary
    -----------------------------  ----------  -----------  -----------------------
    03:44:38:39:be:ef:aa:00:00:01  on          on           remote-vtep: 10.10.10.2
    03:44:38:39:be:ef:bb:00:00:01              on           remote-vtep: 10.10.10.3
                                                            remote-vtep: 10.10.10.4

## nv show evpn vni <vni-id> multihoming bgp-info esi <es-id>

Shows BGP information for a specific multihoming Ethernet segment for the specified VNI.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.
`<es-id>` | The Ethernet segment ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 multihoming bgp-info esi 03:44:38:39:be:ef:aa:00:00:02
                   operational  applied  pending
    -------------  -----------  -------  -------
    [remote-vtep]  10.10.10.2
    type
      local        on
      remote       on

## nv show evpn vni <vni-id> multihoming bgp-info esi <esi-id> remote-vtep

Shows BGP information for a specific multihoming Ethernet segment for the specified VNI.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.
`<es-id>` | The Ethernet segment ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 multihoming esi 03:44:38:39:be:ef:aa:00:00:02 remote-vtep
                flags.ead-per-es  flags.ead-per-evi
    ----------  ----------------  -----------------
    10.10.10.2  on                on

## nv show evpn vni <vni-id> multihoming bgp-info esi <esi-id> remote-vtep <ipv4-address-id>

Shows BGP information for a specific multihoming Ethernet segment for the specified VNI on a specific remote VTEP.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.
`<es-id>` | The Ethernet segment ID.
`<ipv4-address-id>` | The IPv4 address of the remote VTEP.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 multihoming bgp-info esi 03:44:38:39:be:ef:aa:00:00:01 remote-vtep 10.10.10.2
                   operational  applied  pending
    -------------  -----------  -------  -------
    flags
      ead-per-es   on
      ead-per-evi  on

## nv show evpn vni <vni-id> multihoming esi

Shows the EVPN multihoming ESIs for the specified VNI.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 multihoming esi
                                   type.local  type.remote
    -----------------------------  ----------  -----------
    03:44:38:39:be:ef:aa:00:00:01  on

## nv show evpn vni <vni-id> multihoming esi <es-id>

Shows information for a specific multihoming Ethernet segment for the specified VNI.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.
`<es-id>` | The Ethernet segment ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 multihoming esi 03:44:38:39:be:ef:aa:00:00:02

## nv show evpn vni <vni-id> route-advertise

Shows route advertisement information for the specified VNI.

In Cumulus Linux 5.3 and earlier, this command is `nv show evpn evi <vni-id> route-advertise`

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 route-advertise
                     operational  applied  pending
    ---------------  -----------  -------  -------
    default-gateway  off
    svi-ip           off

## nv show evpn vni <vni-id> route-target

Shows route target information for the specified VNI.

In Cumulus Linux 5.3 and earlier, this command is `nv show evpn evi <vni-id> route-target`

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 route-target

## nv show evpn vni <vni-id> route-target both

Shows both import and export route target information for the specified EVPN VNI.

In Cumulus Linux 5.3 and earlier, this command is `nv show evpn evi <vni-id> route-target both`

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 route-target both

## nv show evpn vni <vni-id> route-target both <rt-id>

Shows information about both the specified import and export route target for the specified EVPN VNI.

In Cumulus Linux 5.3 and earlier, this command is `nv show evpn evi <vni-id> route-target both <rt-id>`

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.
`<rt-id>` | The route target ID.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 route-target both 65101:10

## nv show evpn vni <vni-id> route-target export

Shows export route target information for the specified EVPN VNI.

In Cumulus Linux 5.3 and earlier, this command is `nv show evpn evi <vni-id> route-target export`

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 route-target export

## nv show evpn vni <vni-id> route-target export <rt-id>

Shows configuration information about a specific export route target for the specified EVPN VNI.

In Cumulus Linux 5.3 and earlier, this command is `nv show evpn evi <vni-id> route-target export <rt-id>`

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.
`<rt-id>` | The route target ID.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 route-target export 65101:10

## nv show evpn vni <vni-id> route-target import

Shows import route target configuration for the specified EVPN VNI.

In Cumulus Linux 5.3 and earlier, this command is `nv show evpn evi <vni-id> route-target import`

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 route-target import

## nv show evpn vni <vni-id> route-target import <rt-id>

Shows configuration information about a specific import route target for the specified EVPN VNI.

In Cumulus Linux 5.3 and earlier, this command is `nv show evpn evi <vni-id> route-target import <rt-id>`

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.
`<rt-id>` | The route target ID.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 route-target import 65102:10

## nv show evpn vni <vni-id> remote-vtep

Shows the remote VTEPs that connect to the switch.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.6.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 remote-vtep
               flood
    ---------  -----
    10.0.1.34  HER

## nv show interface <interface-id> evpn

Shows EVPN control plane configuration for the specified interface.

### Command Syntax

Syntax | Description
--- | ---
`<interface-id>` | The interface name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show interface bond1 evpn
                       applied            pending
    -----------------  -----------------  -----------------
    multihoming
      uplink           off                off
      segment
        enable         on                 on
        df-preference  50000              50000
        local-id       1                  1
        mac-address    44:38:39:BE:EF:AA  44:38:39:BE:EF:AA

## nv show interface <interface-id> evpn multihoming

Shows the EVPN multihoming interface configuration parameters.

### Command Syntax

Syntax | Description
--- | ---
`<interface-id>` | The interface name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show interface bond1 evpn multihoming
                     operational  applied            pending
    ---------------  -----------  -----------------  -----------------
    uplink                        off                off
    segment
      enable                      on                 on
      df-preference               50000              50000
      local-id                    1                  1
      mac-address                 44:38:39:BE:EF:AA  44:38:39:BE:EF:AA

## nv show interface <interface-id> evpn multihoming segment

Shows EVPN multihoming interface segment configuration.

### Command Syntax

Syntax | Description
--- | ---
`<interface-id>` | The interface name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show interface bond1 evpn multihoming segment
                   operational  applied            pending
    -------------  -----------  -----------------  -----------------
    enable                      on                 on
    df-preference               50000              50000
    local-id                    1                  1
    mac-address                 44:38:39:BE:EF:AA  44:38:39:BE:EF:AA

## nv show vrf <vrf-id> evpn

Shows EVPN control plane configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf RED evpn
                        operational        applied  pending
    ------------------  -----------------  -------  -------
    enable                                 on       on
    vlan                220                auto     auto
    [vni]               4001               4001     4001
    router-mac          44:38:39:22:01:7a
    state               Up
    svi                 vlan220_l3
    system-mac          44:38:39:22:01:7a
    vxlan-interface     vxlan99
    prefix-routes-only  off                off      off

## nv show vrf <vrf-id> evpn bgp-info

Shows layer 3 VNI information from BGP.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf RED evpn bgp-info
                           operational        applied  pending
    ---------------------  -----------------  -------  -------
    local-vtep             10.0.0.1
    rd                     10.10.10.1:6
    router-mac             44:38:39:22:01:7a
    system-ip              10.10.10.1
    system-mac             44:38:39:22:01:7a
    [export-route-target]  65101:4001
    [import-route-target]  65101:4001

## nv show vrf <vrf-id> evpn nexthop-vtep

Shows the EVPN next hop VTEP for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf RED evpn nexthop-vtep
    Nexthop     router-mac
    ----------  -----------------
    10.10.10.2  44:38:39:22:01:78
    10.10.10.3  44:38:39:22:01:84
    10.10.10.4  44:38:39:22:01:8a

## nv show vrf <vrf-id> evpn nexthop-vtep <nexthop-vtep-id>

Shows information about a specific EVPN next hop VTEP in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<nexthop-vtep-id>` | The IP address of the nexthop VTEP.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf RED evpn nexthop-vtep 10.10.10.2
                operational        applied  pending
    ----------  -----------------  -------  -------
    router-mac  44:38:39:22:01:78

## nv show vrf <vrf-id> evpn remote-router-mac

Shows the EVPN remote router MAC addresses in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf RED evpn remote-router-mac
    MAC address        remote-vtep
    -----------------  -----------
    44:38:39:22:01:8a  10.10.10.4
    44:38:39:22:01:78  10.10.10.2
    44:38:39:22:01:84  10.10.10.3

## nv show vrf <vrf-id> evpn remote-router-mac <mac-address>

Shows information about a specific EVPN remote router MAC address in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<mac-address>` | The MAC address.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf RED evpn remote-router-mac 44:38:39:22:01:8a
                 operational  applied  pending
    -----------  -----------  -------  -------
    remote-vtep  10.10.10.4

## nv show vrf <vrf-id> evpn vni

Shows all EVPN VNIs in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf RED evpn vni

    ----
    4001