# BFD

## nv show interface <interface-id> router ospf bfd

Shows the BFD configuration profile associated with the OSPF interface.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.15.0

### Example

    cumulus@switch:~$ nv show interface swp1 router ospf bfd
             operational  applied
    -------  -----------  -------
    profile               BFD1

## nv show interface <interface-id> router pim bfd

Shows the BFD configuration profile associated with the PIM interface.

### Command Syntax

Syntax | Description
--- | ---
`<interface-id>` | The PIM interface.

### Version History

Introduced in Cumulus Linux 5.15.0

### Example

    cumulus@switch:~$ nv show interface vlan10 router pim bfd
             operational  applied
    -------  -----------  -------
    profile               BFD1

## nv show router bfd profile <profile-name>

Shows BFD configuration profile details.

### Command Syntax

Syntax | Description
--- | ---
`<interface-id>` | The interface name.

### Version History

Introduced in Cumulus Linux 5.15.0

### Example

    cumulus@switch:~$ nv show router bfd profile BFD1
                       applied
    -----------------  --------
    detect-multiplier  10
    min-rx-interval    100
    min-tx-interval    100
    shutdown           enabled
    passive-mode       enabled
    minimum-ttl        1

## nv show vrf <vrf-id> router bfd peers

Shows BFD peer information for the VRF.

You can use the following command options:

- `--view brief` shows summarized information.
- `--view standard` shows detailed information
- `--view counters` shows counters, such as the control packet input and output, the echo packet input and output, and if the session is up or down.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.15.0

### Example

    cumulus@switch:~$ nv show vrf default router bfd peers --view brief
    MHop - Multihop, Local - Local, Peer - Peer, Interface - Interface, State -
    State, Passive - Passive Mode, Time - Up/Down Time, Type - Config Type
    LocalId     MHop   Local       Peer        Interface  State  Passive  Time        Type
    ----------  -----  ----------  ----------  ---------  -----  -------  ----------  -------
    20162981    True   6.0.0.24    6.0.0.26               up     False    1:00:08:20  dynamic
    1002134429  True   6000::24    6000::26               up     False    1:00:08:20  dynamic
    1987835266  False  fe80::a288  fe80::9e05  p0_if.100  up     False    1:00:08:20  dynamic
    2124581159  False  fe80::a288  fe80::9e05  p0_if.101  up     False    1:00:08:20  dynamic
    2323511220  True   6000::24    6000::23               up     False    1:00:08:20  dynamic
    4089962224  True   6.0.0.24    6.0.0.23               up     False    0:19:07:20  dynamic

## nv show vrf <vrf-id> router bfd peers <local-id>

Shows BFD peer information for the specified vrf and session.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<local-ID>` | The session ID (integer).

### Version History

Introduced in Cumulus Linux 5.15.0

### Example

    cumulus@switch:~$ nv show vrf default router bfd peers 2

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> bfd

Shows the BFD configuration profile associated with a BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The neighbor ID.

### Version History

Introduced in Cumulus Linux 5.15.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 bfd
             operational  applied
    -------  -----------  -------
    profile               BFD1

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> bfd

Shows the BFD configuration profile associated with a BGP peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.15.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group underlay bfd
    No Data

## nv show vrf <vrf-id> router static <ipv4-address> via <ipv4-address> bfd

Shows the BFD configuration profile associated static routes.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF ID.

### Version History

Introduced in Cumulus Linux 5.15.0

### Example

    cumulus@switch:~$ nv show vrf default router static 10.10.10.101/32 via 10.0.1.0 bfd
             operational  applied
    -------  -----------  -------
    profile               BFD1

## nv show vrf <vrf-id> router static <ipv4-address> distance <integer> via <ipv4-address> bfd

Shows the BFD configuration profile associated with static routes for the specified number of next hops.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF ID.

### Version History

Introduced in Cumulus Linux 5.15.0

### Example

    cumulus@switch:~$ nv show vrf default router static 10.10.10.101/32 distance 2 via 10.0.1.0 bfd
             operational  applied
    -------  -----------  -------
    profile               BFD1