# Segment Routing

## nv show router segment-routing

Shows if segment routing is enabled, and to show the configured locators and SRv6 segment identifiers.

### Version History

Introduced in Cumulus Linux 5.14.0

### Example

    cumulus@switch:~$ nv show router segment-routing
                  operational   applied
    ------------  --------      --------------------
    srv6
      state       disabled      enabled
      [locator]                 LEAF
    static
      [srv6-sid]                 2001:db8:1:1::100/48

## nv show router segment-routing srv6

Shows SRv6 configuration.

### Version History

Introduced in Cumulus Linux 5.14.0

### Example

    cumulus@switch:~$ nv show router segment-routing srv6
              applied   pending
    ---------  --------  -------
    state      disabled  enabled
    [locator]            LEAF

## nv show router segment-routing srv6 stats

Shows SRv6 counter values.

### Version History

Introduced in Cumulus Linux 5.14.0

### Example

    cumulus@switch:~$ nv show router segment-routing srv6 stats
    Hit Counters
    ------------------------------
    SID                                             Packets
    ---------------------------------------      ----------
    2001:db8:1:1::100/48                                   0
    2001:db8:1:1::101/48                                   0

    Drop Counters
    ------------------------------
    Total no-sid-dropped packets

## nv show router segment-routing srv6 stats sid

Shows counter values for a specific SRv6 segment identifier.

### Version History

Introduced in Cumulus Linux 5.14.0

### Example

    cumulus@switch:~$ nv show router segment-routing srv6 stats sid 2001:db8:1:1::100/48

## nv show router segment-routing srv6 stats no-sid-drops

Shows the number of non-SID dropped packets.

### Version History

Introduced in Cumulus Linux 5.14.0

### Example

    cumulus@switch:~$ nv show router segment-routing srv6 stats no-sid-drops
                            operational
    ----------------------  -----------
    no-sid-dropped-packets  0

## nv show router segment-routing srv6 locator

Shows SRv6 locator configuration.

### Version History

Introduced in Cumulus Linux 5.14.0

### Example

    cumulus@switch:~$ nv show router segment-routing srv6 locator
    No Data

## nv show router segment-routing srv6 locator <locator-name>

Shows the configuration for a specific SRv6 locator.

### Version History

Introduced in Cumulus Linux 5.14.0

### Example

    cumulus@switch:~$ nv show router segment-routing srv6 locator LEAF
                  operational  applied
    ------------  -----------  -------
    prefix                     2001:db8:1:1::/32
    block-length               16
    node-length                16
    func-length                0

## nv show router segment-routing static

Shows static segment routing configuration.

### Version History

Introduced in Cumulus Linux 5.14.0

### Example

    cumulus@switch:~$ nv show router segment-routing static
               applied  pending
    ----------  -------  --------------------
    [srv6-sid]           2001:db8:1:1::100/48

## nv show router segment-routing static srv6-sid

Shows information about a specific SRv6 static segment identifier.

### Version History

Introduced in Cumulus Linux 5.14.0

### Example

    cumulus@switch:~$ nv show router segment-routing static srv6-sid 2001:db8:1:1::100/48
                  applied  pending
    ------------  -------  -------
    locator-name           LEAF
    behavior               uA
    interface              swp1