# BGP

## nv show router bgp

Shows global BGP configuration.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show router bgp
                                    applied      pending
    ------------------------------  -----------  -----------
    enable                          on           on
    autonomous-system               65101        65101
    router-id                       10.10.10.1   10.10.10.1
    policy-update-timer             5            5
    graceful-shutdown               off          off
    wait-for-install                off          off
    graceful-restart
      mode                          helper-only  helper-only
      restart-time                  120          120
      path-selection-deferral-time  360          360
      stale-routes-time             360          360
    convergence-wait
      time                          0            0
      establish-wait-time           0            0
    queue-limit
      input                         10000        10000
      output                        10000        10000

## nv show router bgp convergence-wait

Shows global readonly mode configuration. Readonly mode reduces CPU and network usage when restarting the BGP process.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show router bgp convergence-wait
                         applied
    -------------------  -------
    time                 0
    establish-wait-time  0

## nv show router bgp graceful-restart

Shows global BGP graceful restart configuration. BGP graceful restart minimizes the negative effects that occur when BGP restarts.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show router bgp graceful-restart
                                  applied
    ----------------------------  -----------
    mode                          helper-only
    path-selection-deferral-time  360
    restart-time                  120
    stale-routes-time             360

## nv show router bgp queue-limit

Shows the input and output message queue configuration settings.

### Version History

Introduced in Cumulus Linux 5.7.0

### Example

    cumulus@switch:~$ nv show router bgp queue-limit
            applied
    ------  -------
    input   2048
    output  2048

## nv show vrf <vrf-id> router bgp

Shows a summary of the BGP configuration information for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp
                                  operational  applied        pending
    ----------------------------  -----------  -------------  -------------
    enable                                     on             on
    autonomous-system                          auto           auto
    router-id                     10.10.10.1   auto           auto
    rd                                         none           none
    address-family
      ipv4-unicast
        rib-filter                             none           none
        route-export
          to-evpn
            enable                             off            off
        route-import
          from-vrf
            enable                             off            off
        admin-distance
          external                             20             20
          internal                             200            200
        multipaths
          ebgp                                 64             64
          ibgp                                 64             64
          compare-cluster-length               off            off
        enable                                 on             on
        redistribute
          static
            enable                             off            off
          connected
            enable                             on             on
            metric                             auto           auto
            route-map                          none           none
    ...

## nv show vrf <vrf-id> router bgp address-family

Shows a summary of the BGP configuration information for the specified VRF for all address families: IPv4 unicast, IPv6 unicast, and EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family
                                operational  applied  pending
    --------------------------  -----------  -------  -------
    ipv4-unicast
      rib-filter                             none     none
      route-export
        to-evpn
          enable                             off      off
      route-import
        from-vrf
          enable                             off      off
      admin-distance
        external                             20       20
        internal                             200      200
      multipaths
        ebgp                                 64       64
        ibgp                                 64       64
        compare-cluster-length               off      off
      enable                                 on       on
      redistribute
        static
          enable                             off      off
        connected
          enable                             on       on
          metric                             auto     auto
          route-map                          none     none
        kernel
          enable                             off      off
        ospf
          enable                             off      off
      [network]
      [aggregate-route]
    ipv6-unicast
      enable                                 off      off
    l2vpn-evpn
      enable                                 on       on

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast

Shows a summary of the BGP IPv4 configuration information for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast
                              operational  applied  pending
    ------------------------  -----------  -------  -------
    rib-filter                             none     none
    route-export
      to-evpn
        enable                             off      off
    route-import
      from-vrf
        enable                             off      off
    admin-distance
      external                             20       20
      internal                             200      200
    multipaths
      ebgp                                 64       64
      ibgp                                 64       64
      compare-cluster-length               off      off
    enable                                 on       on
    redistribute
      static
        enable                             off      off
      connected
        enable                             on       on
        metric                             auto     auto
        route-map                          none     none
      kernel
        enable                             off      off
      ospf
        enable                             off      off
    [network]
    [aggregate-route]
    ...

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast admin-distance

Shows the BGP IPv4 admin distances configured for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast admin-distance
              operational  applied
    --------  -----------  -------
    external               20
    internal               200

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast aggregate-route

Shows BGP IPv4 aggregate routes (a range of networks in your routing table aggregated into a single prefix) for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast aggregate-route

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast aggregate-route <aggregate-route-id>

Shows information about a specific BGP IPv4 aggregate route (a range of networks in your routing table aggregated into a single prefix).

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<aggregate-route-id>` | The IPv4 address and route prefix in CIDR notation.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast aggregate-route 10.1.0.0/16
                  applied      pending
    ------------  -----------  ---------
    as-set        on          on
    route-map                 routemap1
    summary-only  on          on

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast conditional-disaggregation

Shows BGP conditional disaggregation configuration.

BGP conditional disaggregation advertises specific prefixes when a failure is detected, while continuing to advertise the aggregate route. Combined with anycast Site-of-Origin (SOO) matching, this triggers peer plane leafs to conditionally originate specific routes to draw traffic instead of using the aggregate route that might lead to an unreachable destination.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast conditional-disaggregation
    No Data

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib

Shows the IPv4 local RIB for the specified VRF.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib
    IPV4 Routes
    ==============
        PathCount - Number of paths present for the prefix, MultipathCount - Number of paths that are part of the ECMP, DestFlags - * - bestpath-exists, w - fib-wait-  for-install, s - fib-suppress, i - fib-installed, x - fib-install-failed, LocalPref - Local Preference, Best - Best path, Reason - Reason for selection

        Prefix           PathCount  MultipathCount  DestFlags        Nexthop  Metric  Weight  LocalPref  Aspath  Best  Reason  Flags
        ---------------  ---------  --------------  ---------------  -------  ------  ------  ---------  ------  ----  ------  -----
        10.0.1.12/32     3          1               bestpath-exists
        10.0.1.34/32     5          4               bestpath-exists
        10.0.1.255/32    5          4               bestpath-exists
        10.10.10.1/32    1          1               bestpath-exists
        10.10.10.2/32    5          1               bestpath-exists
        10.10.10.3/32    5          4               bestpath-exists
        10.10.10.4/32    5          4               bestpath-exists
        10.10.10.63/32   5          4               bestpath-exists
        10.10.10.64/32   5          4               bestpath-exists
        10.10.10.101/32  2          1               bestpath-exists
        10.10.10.102/32  2          1               bestpath-exists
        10.10.10.103/32  2          1               bestpath-exists
        10.10.10.104/32  2          1               bestpath-exists

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route

Shows information about the IPv4 routes in the local RIB.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route
    LocalPref - Local Preference, Best - Best path, Reason - Reason for selection

    IPv4 Prefix      Nexthop  Metric  Weight  LocalPref  Aspath  Best  Reason      Flags
    ---------------  -------  ------  ------  ---------  ------  ----  ---------…  ---------
    10.0.0.9/32      swp51    0                          65103   on    Router ID   multipath
                                                         65199
                     swp52    0                          65103                     multipath
                                                         65199
    10.0.0.10/32     swp51    0                          65103   on    Router ID   multipath
                                                         65199
                     swp52    0                          65103                     multipath
                                                         65199
    10.10.10.1/32             0       32768                      on    First path
                                                                       received
    10.10.10.2/32    swp51    0                          65102                     multipath
                                                         65199
                     swp52    0                          65102   on    Older Path  multipath
                                                         65199
    10.10.10.3/32    swp51    0                          65103                     multipath
                                                         65199
                     swp52    0                          65103   on    Older Path  multipath
                                                         65199
    10.10.10.4/32    swp51    0                          65104                     multipath
                                                         65199
                     swp52    0                          65104   on    Older Path  multipath
                                                         65199
    10.10.10.101/32  swp51    0                          65199   on    First path
                                                                       received

    10.10.10.102/32  swp52    0                          65199   on    First path
                                                                       received

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route <route-id>

Shows information about the specified IPv4 route in the local RIB, such as the BGP neighbor to which the path is advertised and the path count.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route 10.10.10.3/32
                     operational  applied
    ---------------  -----------  -------
    [advertised-to]  swp51
    [advertised-to]  swp52
    [path]           1
    [path]           2
    path-count       2
    multipath-count  1

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route <route-id> path

Shows information about the paths for the specified IPv4 route in the local RIB.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>` command instead.

Add `-o json` at the end of the command to see the output in a more readable format.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route 10.0.0.9/32 path -o json
    {

      "1": {
        "aspath": {
          "65002": {}
        },
        "bestpath": {
          "from-as": 65002,
          "overall": "yes",
          "selection-reason": "First path received"
        },
        "flags": {
          "bestpath": {},
          "valid": {}
        },
        "flags-string": "*v",
        "last-update": "2024-08-05T03:51:08Z",
        "metric": 0,
        "nexthop": {
          "1": {
            "accessible": "on",
            "afi": "ipv6",
            "ip": "fe80::4ab0:2dff:fe08:9898",
            "metric": 0,
            "scope": "global"
          },
          "2": {
            "accessible": "on",
            "afi": "ipv6",
            "ip": "fe80::4ab0:2dff:fe08:9898",
            "scope": "link-local",
            "used": "on"
          }
        },
        "nexthop-count": 2,
        "origin": "incomplete",
        "path-from": "external",
        "peer": {
          "hostname": "spine01",
          "id": "fe80::4ab0:2dff:fe08:9898",
          "interface": "swp51",
          "router-id": "10.10.10.101",
          "type": "external"
        },
        "valid": "on"
      },
      "2": {
        "aspath": {
          "65103": {},
          "65199": {}
        },
        "bestpath": {
          "from-as": 65199,
          "overall": "on",
          "selection-reason": "Older Path"
        },
        "flags": {
          "multipath": {}
        },
        "last-update": 1682960995,
        "nexthop": {
          "1": {
            "accessible": "on",
            "afi": "ipv6",
            "ip": "fe80::4ab0:2dff:fed8:67cb",
            "metric": 0,
            "scope": "global"
          },
          "2": {
            "accessible": "on",
            "afi": "ipv6",
            "ip": "fe80::4ab0:2dff:fed8:67cb",
            "scope": "link-local",
            "used": "on"
          }
        },
        "nexthop-count": 2,
        "origin": "incomplete",
        "path-from": "external",
        "peer": {
          "hostname": "spine02",
          "id": "fe80::4ab0:2dff:fed8:67cb",
          "interface": "swp52",
          "router-id": "10.10.10.102",
          "type": "external"
        },
        "valid": "on"
      }
    }

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route <route-id> path <path-id>

Shows information about a specific IPv4 route path in the local RIB.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>` command instead.

Add `-o json` at the end of the command to see the output in a more readable format.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route 10.0.0.9/32 path 1 -o json
    {

      "1": {
        "aspath": {
          "65002": {}
        },
        "bestpath": {
          "from-as": 65002,
          "overall": "yes",
          "selection-reason": "First path received"
        },
        "flags": {
          "bestpath": {},
          "valid": {}
        },
        "flags-string": "*v",
        "last-update": "2024-08-05T03:51:08Z",
        "metric": 0,
        "nexthop": {
        "1": {
          "accessible": "on",
          "afi": "ipv6",
          "ip": "fe80::4ab0:2dff:fe08:9898",
          "metric": 0,
          "scope": "global"
        },
        "2": {
          "accessible": "on",
          "afi": "ipv6",
          "ip": "fe80::4ab0:2dff:fe08:9898",
          "scope": "link-local",
          "used": "on"
        }
      },
      "nexthop-count": 2,
      "origin": "incomplete",
      "path-from": "external",
      "peer": {
        "hostname": "spine01",
        "id": "fe80::4ab0:2dff:fe08:9898",
        "interface": "swp51",
        "router-id": "10.10.10.101",
        "type": "external"
      },
      "valid": "on"
    }

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route <route-id> path <path-id> aspath

Shows the AS paths for the specified IPv4 route in the local RIB.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route 10.10.10.3/32 path 2 aspath
    Aspath
    ------
    65103
    65199

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route <route-id> path <path-id> bestpath

Shows best path information, such as the selection reason, for the specified IPv4 route in the local RIB.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route 10.10.10.3/32 path 2 bestpath
                      operational  applied
    ----------------  -----------  -------
    from-as           65199
    overall           on
    selection-reason  Older Path

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route <route-id> path <path-id> community

Shows the community names for the community list for the specified IPv4 route path in the local RIB.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route 10.10.10.3/32 path 2 community

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route <route-id> path <path-id> ext-community

Shows the community names for the extended community list for the specified IPv4 route path in the local RIB.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route 10.10.10.3/32 path 2 ext-community

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route <route-id> path <path-id> flags

Shows route path flags for the specified IPv4 route in the local RIB.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route 10.10.10.3/32 path 2 flags
    operational  applied
    -----------  -------
    multipath

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route <route-id> path <path-id> large-community

Shows the community names for the large community list for the specified IPv4 route path in the local RIB.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route 10.10.10.3/32 path 2 large-community

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route <route-id> path <path-id> nexthop

Shows information about the nexthops for the specified IPv4 route path in the local RIB.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route 10.10.10.3/32 path 2 nexthop
    Nexthop  accessible  afi   ip                         metric  scope       used
    -------  ----------  ----  -------------------------  ------  ----------  ----
    1        on          ipv6  fe80::4ab0:2dff:fed8:67cb  0       global
    2        on          ipv6  fe80::4ab0:2dff:fed8:67cb          link-local  on

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route <route-id> path <path-id> nexthop <nexthop-id>

Shows next hop information for the specified IPv4 route path in the local RIB.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation
`<path-id>` | The path ID.
`<nexthop-id>` | The nexthop ID.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route 10.10.10.3/32 path 2 nexthop 2
                operational                applied
    ----------  -------------------------  -------
    ip          fe80::202:ff:fe00:26
    afi         ipv6
    scope       global
    accessible  on
    metric      0

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast loc-rib route <route-id> path <path-id> peer

Shows BGP neighbor information for the specified IPv4 route path in the local RIB.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast loc-rib route 10.10.10.3/32 path 2 peer
               operational                applied
    ---------  -------------------------  -------
    hostname   spine02
    id         fe80::4ab0:2dff:fed8:67cb
    interface  swp52
    router-id  10.10.10.102
    type       external

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast multipaths

Shows BGP IPv4 multipath configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast multipaths
                            operational  applied
    ----------------------  -----------  -------
    compare-cluster-length               off
    ebgp                                 64
    ibgp                                 64

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast network

Shows BGP IPv4 static networks for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast network
    No Data

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast network <static-network-id>

Shows information about a specific BGP IPv4 static network for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<static-network-id>` | The IPv4 address and route prefix in CIDR notation.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast network 10.10.10.101/32
               operational  applied
    ---------  -----------  -------
    route-map               HI-PRIO

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast redistribute

Shows configuration information for BGP IPv4 route redistribution for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast redistribute
                 applied  pending
    -----------  -------  -------
    static
      enable     off      off
    connected
      enable     on       on
      metric     auto     auto
      route-map  none     none
    kernel
      enable     off      off
    ospf
      enable     off      off

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast redistribute connected

Shows configuration information for BGP IPv4 connected route redistribution for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast redistribute connected
               applied  pending
    ---------  -------  -------
    enable     on       on
    metric     auto     auto
    route-map  none     none

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast redistribute kernel

Shows configuration information for BGP IPv4 kernel route redistribution for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast redistribute kernel
            applied  pending
    ------  -------  -------
    enable  off      off

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast redistribute ospf

Shows configuration information for redistributing OSPF IPv4 routes into BGP for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast redistribute ospf
            applied  pending
    ------  -------  -------
    enable  off      off

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast redistribute static

Shows configuration information for IPv4 BGP static route redistribution for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast redistribute static
            applied  pending
    ------  -------  -------
    enable  off      off

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast route

Shows the BGP IPv4 routing table.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.11.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast route
    PathCount - Number of paths present for the prefix, MultipathCount - Number of
    paths that are part of the ECMP, DestFlags - * - bestpath-exists, w - fib-wait-
    for-install, s - fib-suppress, i - fib-installed, x - fib-install-failed

    Prefix           PathCount  MultipathCount  DestFlags
    ---------------  ---------  --------------  ---------
    10.0.1.12/32     2          1               *
    10.0.1.34/32     5          4               *
    10.0.1.255/32    5          4               *
    10.10.10.1/32    1          1               *
    10.10.10.2/32    5          1               *
    10.10.10.3/32    5          4               *
    10.10.10.4/32    5          4               *
    10.10.10.63/32   5          4               *
    10.10.10.64/32   5          4               *
    10.10.10.101/32  2          1               *
    10.10.10.102/32  2          1               *
    10.10.10.103/32  2          1               *
    10.10.10.104/32  2          1               *

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast route <route-id>

Shows information about the BGP IPv4 route.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 address and route prefix in CIDR notation.

### Version History

Introduced in Cumulus Linux 5.11.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast route 10.10.10.3/32
                     operational
    ---------------  -----------
    path-count       5
    multipath-count  4

    path
    =======

        Origin - Route origin, Local - Locally originated route, Sourced - Sourced
        route, Weight - Route weight, Metric - Route metric, LocalPref - Route local
        preference, PathFrom - Route path origin, LastUpdate - Route last update,
        NexthopCnt - Number of nexthops, Flags - = - multipath, * - bestpath, v - valid,
        s - suppressed, R - removed, S - stale

        Path  Origin      Local  Sourced  Weight  Metric  LocalPref  PathFrom  LastUpdate            NexthopCnt  Flags
        ----  ----------  -----  -------  ------  ------  ---------  --------  --------------------  ----------  -----
        1     incomplete                                             external  2024-11-23T12:58:55Z  2           =*v
        2     incomplete                                             external  2024-11-23T12:59:04Z  2           =v
        3     incomplete                                             external  2024-11-23T12:58:55Z  2           =v
        4     incomplete                                             external  2024-11-23T12:59:03Z  2           =v
        5     incomplete                                             external  2024-11-23T12:59:03Z  2           *v

    advertised-to
    ================
        Neighbor       hostname
        -------------  --------
        peerlink.4094  leaf02
        swp51          spine01
        swp52          spine02
        swp53          spine03
        swp54          spine04

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast route-count

Shows the BGP IPv4 route and path count.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.11.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast route-count
                  operational  applied
    ------------  -----------  -------
    total-routes  13           13
    total-paths   46           46

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast route-export

Shows BGP IPv4 route export configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast route-export
                    operational  applied
    --------------  -----------  -------
    to-evpn
      enable                     off
    to-vrf
      [list]        none
    [route-target]  none
    rd              none

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast route-export to-evpn

Shows configuration for IPv4 prefix-based routing using EVPN type-5 routes. Type-5 routes (or prefix routes) primarily route to destinations outside of the data center fabric. EVPN prefix routes carry the layer 3 VNI and router MAC address and follow the symmetric routing model to route to the destination prefix.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast route-export to-evpn
    route-export to-evpn
            operational  applied
    ------  -----------  -------
    enable               off

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast route-import

Shows configuration information about BGP IPV4 route import (route leaking) for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast route-import
                    operational  applied
    --------------  -----------  -------
    from-vrf
      enable                     off
      [list]        none
    [route-target]  none

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast route-import from-vrf

Shows configuration information about VRF to VRF IPv4 route leaking.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast route-import from-vrf
           operational  applied
    ------  -----------  -------
    enable               off
    [list]  none

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast route-import from-vrf list

Shows the IPv4 routes in the BGP RIB imported from the VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast route-import from-vrf list
    ----
    none

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast route-import from-vrf list <leak-vrf-id>

Shows IPv4 routes in the BGP RIB that leak between VRFs.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<leak-vrf-id>` | The VRF from which routes are leaked.

### Version History

Introduced in Cumulus Linux 5.1.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast route-import from-vrf list BLUE
    ----
    none

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast soo-route

Shows the BGP Site-of-Origin routes.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.8.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast soo-route

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast soo-route <ip-address>

Shows information about the specific BGP Site-of-Origin route.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<ip-address>` | The IP address.

### Version History

Introduced in Cumulus Linux 5.8.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast soo-route 10.10.10.5

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast update-group

Shows the BGP IPv4 update groups for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast update-group

     RouteMap - Outbound route map, MinAdvInterval - Minimum route advertisement
    interval, CreationTime - Time when the update group was created, LocalAsChange -
    LocalAs changes for inbound route, Flags - r - replace-as, x - no-prepend

    UpdateGrp  RouteMap  MinAdvInterval  CreationTime          LocalAsChange  Flags
    ---------  --------  --------------  --------------------  -------------  -----
    1                    1               2024-08-05T03:51:08Z

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast update-group <group-id>

Shows information about a specific BGP IPv4 update group in the specified VRF.

In Cumulus Linux 5.10 and earlier, add `-o json` at the end of the command to see the output in a more readable format.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<group-id>` | The group ID.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast update-group 1
                                      operational
    --------------------------------  --------------------
    update-group-id                   1
    min-route-advertisement-interval  0
    create-time                       2024-11-15T10:01:47Z

    sub-group
    ============

        CreateTime - Time when the sub group was created, AdvRouteCnt - Number of routes
        advertised to peer, Refresh - Indicates if subgroup requires refresh,
        TotalQueuePkt - Total packets in queue, TotalEnqueuePkt - Total packets
        enqueued, PktQueueLength - Packet queue length, Neighbor - Sub group peer info

        GrpID  CreateTime            AdvRouteCnt  Refresh  TotalQueuePkt  TotalEnqueuePkt  PktQueueLength  Neighbor
        -----  --------------------  -----------  -------  -------------  ---------------  --------------  -------------
        1      2024-11-15T10:01:47Z  13           off      31             31               0               peerlink.4094
                                                                                                           swp52
                                                                                                           swp53
                                                                                                           swp54

## nv show vrf <vrf-id> router bgp address-family ipv4-unicast update-group <group-id> sub-group

Shows the subgroups for a specific BGP IPv4 update group in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<group-id>` | The group ID.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unicast update-group 1 sub-group

    CreateTime - Time when the sub group was created, AdvRouteCnt - Number of routes
    advertised to peer, Refresh - Indicates if subgroup requires refresh,
    TotalQueuePkt - Total packets in queue, TotalEnqueuePkt - Total packets
    enqueued, PktQueueLength - Packet queue length, Neighbor - Sub group peer info

    GrpID  CreateTime            AdvRouteCnt  Refresh  TotalQueuePkt  TotalEnqueuePkt  PktQueueLength  Neighbor
    -----  --------------------  -----------  -------  -------------  ---------------  --------------  -------------
    1      2024-11-15T10:01:47Z  13           off      31             31               0               peerlink.4094
                                                                                                       swp52
                                                                                                       swp53
                                                                                                       swp54

## nv show vrf <vrf-id> router bgp address-family ipv4-unreachability

Shows if BGP unreachability is enabled on the switch.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unreachability
           operational  applied
    -----  -----------  ----------------
    state               enabled
                        state
                        advertise-origin

## nv show vrf router bgp address-family ipv4-unreachability advertise-origin

Shows the BGP unreachability advertise-origin configuration.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unreachability advertise-origin

## nv show vrf router bgp address-family ipv4-unreachability advertise-unreach

Shows the BGP unreachability aggregate prefix and the included interfaces for which unreachability is conditionally advertised.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unreachability advertise-unreach
                        operational      applied
    ------------------  -------------    -------------
    [interfaces-match]  10.10.10.101/32  10.10.10.101/32

## nv show vrf router bgp address-family ipv4-unreachability advertise-unreach interfaces-match

Shows the interfaces for which unreachability is conditionally advertised.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv6-unreachability advertise-unreach interfaces-match
    -------------
    10.10.10.101/32

## nv show vrf <vrf-id> router bgp address-family ipv4-unreachability route

Shows BGP unreachability routes.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unreachability route
    PathCount - Number of paths present for the prefix, MultipathCount - Number of
    paths that are part of the ECMP, DestFlags - * - bestpath-exists, w - fib-wait-
    for-install, s - fib-suppress, i - fib-installed, x - fib-install-failed

    Prefix            PathCount  MultipathCount  DestFlags
    ----------------  ---------  --------------  ---------
    10.10.10.101/32   4          0               *

## nv show vrf <vrf-id> router bgp address-family ipv4-unreachability route <route-id>

Shows information about the specified BGP unreachability route.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IPv4 route.

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unreachability route 10.10.10.101/32

## nv show vrf <vrf-id> router bgp address-family ipv4-unreachability route-count

Shows the BGP unreachability route count.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family ipv4-unreachability route-count
                 operational
    -----------  -----------
    total-paths  1

## nv show vrf <vrf-id> router bgp confederation

Shows BGP confederation configuration. To reduce the number of iBGP peerings, configure a confederation to divide an AS into a smaller sub-AS.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.8.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp confederation
                 operational  applied
    -----------  -----------  -----------
    id                        2
    [member-as]               65101-65104

## nv show vrf <vrf-id> router bgp confederation member-as

Shows the BGP confederation member AS. A BGP confederation divides a large AS into subautonomous systems, which are uniquely identified by a sub-AS number.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.8.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp confederation member-as
    No Data

## nv show vrf <vrf-id> router bgp dynamic-neighbor

Shows BGP dynamic neighbor configuration on the switch. BGP dynamic neighbors provide BGP peering to remote neighbors within a specified range of IPv4 or IPv6 addresses for a BGP peer group. You can configure each range as a subnet IP address.

After you configure the dynamic neighbors, a BGP speaker can listen for, and form peer relationships with, any neighbor that is in the IP address range and maps to a peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.3.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp dynamic-neighbor
    [listen-range]               10.0.1.0/24
    limit                        5

## nv show vrf <vrf-id> router bgp dynamic-neighbor listen-range

Shows the address range configuration for BGP peering to remote neighbors.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.3.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp dynamic-neighbor listen-range
    No Data

## nv show vrf <vrf-id> router bgp dynamic-neighbor listen-range <ip-sub-prefix-id>

Shows information about a specific address range for BGP peering to remote neighbors.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<ip-sub-prefix-id>` | The address range.

### Version History

Introduced in Cumulus Linux 5.3.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp dynamic-neighbor listen-range 10.0.1.0/24
                operational  applied
    ----------  -----------  -------
    peer-group               SPINE

## nv show vrf <vrf-id> router bgp neighbor

Shows information about all BGP neighbors.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor
    AS - Remote Autonomous System, PeerEstablishedTime - Peer established time in
    UTC format, UpTime - Uptime in milliseconds, Afi-Safi - Address family, PfxSent
    - Transmitted prefix counter, PfxRcvd - Recieved prefix counter

    Neighbor       AS     State        PeerEstablishedTime   UpTime   MsgRcvd  MsgSent Afi-Safi      PfxSent  PfxRcvd
    -------------  -----  -----------  --------------------  -------  -------  ------- ------------  -------  -------
    peerlink.4094  65102  established  2024-11-23T12:58:56Z  2136000  800      787 ipv4-unicast  13       12
     l2vpn-evpn    63       45
    swp51          65199  established  2024-11-23T12:58:54Z  2136000  803      786 ipv4-unicast  13       8
     l2vpn-evpn    63       45
    swp52          65199  established  2024-11-23T12:59:02Z  2136000  797      782 ipv4-unicast  13       8
     l2vpn-evpn    63       45
    swp53          65199  established  2024-11-23T12:58:54Z  2136000  803      786 ipv4-unicast  13       8
     l2vpn-evpn    63       45
    swp54          65199  established  2024-11-23T12:59:01Z  2136000  797      783 ipv4-unicast  13       8
     l2vpn-evpn    63       45

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id>

Shows global configuration and statistics for the specified BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51
                                   operational                applied
    -----------------------------  -------------------------  ---------------------------------------
    password                                                  $nvsec$d1a028e8c7f97db92876c2a30fcc403f
    enforce-first-as                                          off
    passive-mode                                              off
    nexthop-connected-check                                   on
    description                                               none
    bfd
      enable                                                  off
    ttl-security
      enable                       on                         off
      hops                         1
    local-as
      enable                                                  off
    timers
      keepalive                    3                          auto
      hold                         9                          auto
      connection-retry             10                         auto
      route-advertisement          none                       auto
    address-family
      ipv4-unicast
        enable                                                on
        route-reflector-client                                off
        soft-reconfiguration                                  off
        nexthop-setting                                       auto
        add-path-tx                                           off
        attribute-mod
          aspath                   off                        on
          med                      off                        on
          nexthop                  off                        on
        aspath
          replace-peer-as                                     off
          private-as                                          none
          allow-my-asn
            enable                                            off
        graceful-restart
          rx-eof-rib               off
          tx-eof-rib               off
        weight                                                0
        community-advertise
          regular                  on                         on
          extended                 on                         on
          large                    off                        off
        conditional-advertise
          enable                                              off
        policy
          inbound
            route-map                                         none
            prefix-list                                       none
            aspath-list                                       none
    ...

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family

Shows all address family configuration for the specified BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family
                                 operational  applied
    ---------------------------  -----------  -------
    ipv4-unicast
      enable                                  on
      route-reflector-client                  off
      soft-reconfiguration                    off
      nexthop-setting                         auto
      add-path-tx                             off
      attribute-mod
        aspath                   off          on
        med                      off          on
        nexthop                  off          on
      aspath
        replace-peer-as                       off
        private-as                            none
        allow-my-asn
          enable                              off
      graceful-restart
        rx-eof-rib               off
        tx-eof-rib               off
      weight                                  0
      community-advertise
        regular                  on           on
        extended                 on           on
        large                    off          off
      conditional-advertise
        enable                                off
    ...

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast

Shows configuration information for the specified BGP IPv4 neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast
                               operational  applied
    -------------------------  -----------  -------
    enable                                  on
    route-reflector-client                  off
    route-server-client                     off
    soft-reconfiguration                    off
    nexthop-setting                         auto
    add-path-tx                             off
    attribute-mod
      aspath                   off          on
      med                      off          on
      nexthop                  off          on
    aspath
      replace-peer-as                       off
      private-as                            none
      allow-my-asn
        enable                              off
    graceful-restart
      rx-eof-rib               off
      tx-eof-rib               off
    weight                                  0
    ...

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes

Shows information about the IPv4 advertised routes for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast advertised-routes
    PathCount - Number of paths present for the prefix, MultipathCount - Number of
    paths that are part of the ECMP

    IPv4 Prefix      PathCount  MultipathCount  DestFlags
    ---------------  ---------  --------------  ---------------
    10.0.1.12/32     2          1               bestpath-exists
    10.0.1.34/32     5          4               bestpath-exists
    10.0.1.255/32    5          4               bestpath-exists
    10.10.10.1/32    1          1               bestpath-exists
    10.10.10.2/32    5          1               bestpath-exists
    10.10.10.3/32    5          4               bestpath-exists
    10.10.10.4/32    5          4               bestpath-exists
    10.10.10.63/32   5          4               bestpath-exists
    10.10.10.64/32   5          4               bestpath-exists
    10.10.10.101/32  2          1               bestpath-exists
    10.10.10.102/32  2          1               bestpath-exists
    10.10.10.103/32  2          1               bestpath-exists
    10.10.10.104/32  2          1               bestpath-exists

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes <route-id>

Shows information about a specific IPv4 advertised route for a BGP neighbor in the specified VRF.

In Cumulus Linux 5.10 and earlier, add `-o json` at the end of the command to see the output in a more readable format.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 advertised route.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp52 address-family ipv4-unicast advertised-routes 10.10.10.3/32
                     operational
    ---------------  -----------
    path-count       4
    multipath-count  3

    path
    =======

        Origin - Route origin, Local - Locally originated route, Sourced - Sourced
        route, Weight - Route weight, Metric - Route metric, LocalPref - Route local
        preference, PathFrom - Route path origin, LastUpdate - Route last update,
        NexthopCnt - Number of nexthops, Flags - = - multipath, * - bestpath, v - valid,
        s - suppressed, R - removed, S - stale

        Path  Origin      Local  Sourced  Weight  Metric  LocalPref  PathFrom  LastUpdate            NexthopCnt  Flags
        ----  ----------  -----  -------  ------  ------  ---------  --------  --------------------  ----------  -----
        1     incomplete                                             external  2024-11-15T10:03:31Z  2           =*v
        2     incomplete                                             external  2024-11-15T10:03:26Z  2           =v
        3     incomplete                                             external  2024-11-15T10:03:26Z  2           =v
        4     incomplete                                             external  2024-11-15T10:03:23Z  2           *v
    ...

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes <route-id> path

Shows path information about a specific IPv4 advertised route for a BGP neighbor in the specified VRF.

In Cumulus Linux 5.10 and earlier, add `-o json` at the end of the command to see the output in a more readable format.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 advertised route.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp52 address-family ipv4-unicast advertised-routes 10.10.10.3/32 path

    Origin - Route origin, Local - Locally originated route, Sourced - Sourced
    route, Weight - Route weight, Metric - Route metric, LocalPref - Route local
    preference, PathFrom - Route path origin, LastUpdate - Route last update,
    NexthopCnt - Number of nexthops, Flags - = - multipath, * - bestpath, v - valid,
    s - suppressed, R - removed, S - stale

    Path  Origin      Local  Sourced  Weight  Metric  LocalPref  PathFrom  LastUpdate            NexthopCnt  Flags
    ----  ----------  -----  -------  ------  ------  ---------  --------  --------------------  ----------  -----
    1     incomplete                                             external  2024-11-15T10:03:31Z  2           =*v
    2     incomplete                                             external  2024-11-15T10:03:26Z  2           =v
    3     incomplete                                             external  2024-11-15T10:03:26Z  2           =v
    4     incomplete                                             external  2024-11-15T10:03:23Z  2           *v

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes <route-id> path <path-id>

Shows information about a specific IPv4 advertised route path ID for a BGP neighbor in the specified VRF.

In Cumulus Linux 5.10 and earlier, add `-o json` at the end of the command to see the output in a more readable format.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 advertised route.
`<path-id>` | The IPv4 advertised route path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp52 address-family ipv4-unicast advertised-routes 10.10.10.3/32 path 1
                        operational
    ------------------  ------------------------
    origin              incomplete
    valid               on
    path-from           external
    last-update         2024-11-15T10:03:31Z
    nexthop-count       2
    flags-string        =*v
    peer
      id                fe80::4ab0:2dff:fe5e:6ad
      router-id         10.10.10.102
      hostname          spine02
      interface         swp52
      type              external
    bestpath
      from-as           65199
      overall           yes
      selection-reason  AS Path

    nexthop
    ==========
        Nexthop  accessible  afi   ip                        metric  scope       used
        -------  ----------  ----  ------------------------  ------  ----------  ----
        1        on          ipv6  fe80::4ab0:2dff:fe5e:6ad  0       global
        2        on          ipv6  fe80::4ab0:2dff:fe5e:6ad          link-local  on

    aspath
    =========
        Aspath
        ------
        65103
        65199

    community
    ============
    No Data

    ext-community
    ================
    No Data

    large-community
    ==================
    No Data

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes <route-id> path <path-id> aspath

Shows information about the AS path for an IPv4 advertised route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 advertised route.
`<path-id>` | The IPv4 advertised route path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp52 address-family ipv4-unicast advertised-routes 10.10.10.3/32 path 1 aspath
    Aspath
    ------
    65103
    65199

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes <route-id> path <path-id> bestpath

Shows information about the bestpath for an IPv4 advertised route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 advertised route.
`<path-id>` | The IPv4 advertised route path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp52 address-family ipv4-unicast advertised-routes 10.10.10.3/32 path 1 bestpath
                      operational
    ----------------  -----------
    from-as           65199
    overall           yes
    selection-reason  AS Path

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes <route-id> path <path-id> community

Shows information about the communities for an IPv4 advertised route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 advertised route.
`<path-id>` | The IPv4 advertised route path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast advertised-routes 10.10.10.101/32 path 1 community
    No Data

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes <route-id> path <path-id> ext-community

Shows information about the extended communities for an IPv4 advertised route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 advertised route.
`<path-id>` | The IPv4 advertised route path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast advertised-routes 10.10.10.1/32 path 1 ext-community
    No Data

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes <route-id> path <path-id> flags

Shows information about the flags for an IPv4 advertised route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 advertised route.
`<path-id>` | The IPv4 advertised route path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp52 address-family ipv4-unicast advertised-routes 10.10.10.3/32 path 1 flags
    operational
    -----------
    multipath
    bestpath
    valid

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes <route-id> path <path-id> large-community

Shows information about the large communities for an IPv4 advertised route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 advertised route.
`<path-id>` | The IPv4 advertised route path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast advertised-routes 10.10.10.1/32 path 1 large-community
    No Data

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes <route-id> path <path-id> nexthop

Shows information about the next hops for an IPv4 advertised route path ID for a BGP neighbor in the specified VRF.

In Cumulus Linux 5.10 and earlier, add `-o json` at the end of the command to see the output in a more readable format.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 advertised route.
`<path-id>` | The IPv4 advertised route path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp52 address-family ipv4-unicast advertised-routes 10.10.10.3/32 path 1 nexthop
    Nexthop  accessible  afi   ip                        metric  scope       used
    -------  ----------  ----  ------------------------  ------  ----------  ----
    1        on          ipv6  fe80::4ab0:2dff:fe5e:6ad  0       global
    2        on          ipv6  fe80::4ab0:2dff:fe5e:6ad          link-local  on

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes <route-id> path <path-id> nexthop <nexthop-id>

Shows information about a specific next hop for an IPv4 advertised route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 advertised route.
`<path-id>` | The IPv4 advertised route path ID.
`<nexthop-id>` | The nexthop ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp52 address-family ipv4-unicast advertised-routes 10.10.10.3/32 path 1 nexthop 1
                operational
    ----------  ------------------------
    ip          fe80::4ab0:2dff:fe5e:6ad
    afi         ipv6
    scope       global
    accessible  on
    metric      0

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast advertised-routes <route-id> path <path-id> peer

Shows information about the peers for an IPv4 advertised route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 advertised route.
`<path-id>` | The IPv4 advertised route path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp52 address-family ipv4-unicast advertised-routes 10.10.10.3/32 path 1 peer
               operational
    ---------  ------------------------
    id         fe80::4ab0:2dff:fe5e:6ad
    router-id  10.10.10.102
    hostname   spine02
    interface  swp52
    type       external

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast aspath

Shows the configuration settings for handling the AS path for prefixes to and from the specified BGP IPv4 neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast aspath
                     applied
    ---------------  -------
    replace-peer-as  off
    private-as       none
    allow-my-asn
      enable         off

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast aspath allow-my-asn

Shows if it is acceptable for a received AS path from the specified IPv4 neighbor to contain the ASN of the local system.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast aspath allow-my-asn
            applied
    ------  -------
    enable  off

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast attribute-mod

Shows the attribute modification configuration settings for the specified BGP IPv4 neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast attribute-mod
              operational  applied
    -------  -----------  -------
    aspath   off          on
    med      off          on
    nexthop  off          on

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast capabilities

Shows all advertised and received capabilities for the specified BGP IPv4 neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast capabilities
    No Data

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast community-advertise

Shows community advertise configuration information for the specified BGP IPv4 neighbor. The community advertise option determines if the neighbor can advertise a prefix to any iBGP or eBGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast community-advertise
              operational  applied
    --------  -----------  -------
    regular   on           on
    extended  on           on
    large     off          off

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast conditional-advertise

Shows conditional advertisement configuration information for the specified BGP IPv4 neighbor. The BGP conditional advertisement option lets you advertise certain routes only if other routes either do or do not exist.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast conditional-advertise
            operational  applied
    ------  -----------  -------
    enable               off

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast default-route-origination

Shows default route origination configuration for the specified BGP IPv4 neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast default-route-origination
            operational  applied
    ------  -----------  -------
    state                disabled

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast graceful-restart

Shows BGP graceful restart configuration information for the specified BGP IPv4 neighbor. BGP graceful restart minimizes the negative effects that occur when BGP restarts.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast graceful-restart
                operational
    ----------  -----------
    rx-eof-rib  on
    tx-eof-rib  on

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast graceful-restart timers

Shows the BGP graceful restart selection deferral and stale path timer settings for the BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.

### Version History

Introduced in Cumulus Linux 5.9.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast graceful-restart timers
                 operational
    -----------  -----------
    stale-path
      timer-sec  360

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast graceful-restart timers selection-deferral

Shows the BGP graceful restart selection deferral timers for the BGP neighbor.

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.

### Version History

Introduced in Cumulus Linux 5.9.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast graceful-restart timers selection-deferral

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast graceful-restart timers stale-path

Shows the BGP graceful restart stale path timer settings for the BGP neighbor.

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.

### Version History

Introduced in Cumulus Linux 5.9.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast graceful-restart timers stale-path
               operational
    ---------  -----------
    timer-sec  360

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast policy

Shows the policies for the specified BGP IPv4 neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast policy
                      operational  applied
    ----------------  -----------  -------
    inbound
      route-map                    none
      prefix-list                  none
      aspath-list                  none
    outbound
      route-map                    none
      unsuppress-map               none
      prefix-list                  none
      aspath-list                  none

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast policy inbound

Shows the inbound policy for the specified BGP IPv4 neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast policy inbound
                 operational  applied
    -----------  -----------  -------
    route-map                 none
    prefix-list               none
    aspath-list               none

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast policy outbound

Shows the outbound policy for the specified BGP IPv4 neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast policy outbound
                    operational  applied
    --------------  -----------  -------
    route-map                    none
    unsuppress-map               none
    prefix-list                  none
    aspath-list                  none

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast prefix-limits

Shows the limits on prefixes from the specified IPv4 neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast prefix-limits
                         operational  applied
    -------------------  -----------  -------
    inbound
      maximum                         none
      warning-threshold               75
      warning-only       off

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast prefix-limits inbound

Shows the limits on inbound prefixes from the specified IPv4 neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast prefix-limits inbound
                       operational  applied
    -----------------  -----------  -------
    maximum                         none
    warning-threshold               75
    warning-only       off

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes

Shows information about the IPv4 received routes for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes <route-id>

Shows information about a specific IPv4 received route for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 route.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes 10.0.1.2/32

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes <route-id> path

Shows information about a specific IPv4 received route path for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 route.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes 10.0.1.2/32 path

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes <route-id> path <path-id>

Shows information about a specific IPv4 received route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 route.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes 10.0.1.2/32 path 1

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes <route-id> path <path-id> aspath

Shows information about the AS paths for a specific IPv4 received route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 route.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes 10.0.1.2/32 path 1 aspath

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes <route-id> path <path-id> bestpath

Shows information about the best paths for a specific IPv4 received route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 route.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes 10.0.1.2/32 path 1 bestpath -o json

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes <route-id> path <path-id> community

Shows information about the communities for a specific IPv4 received route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 route.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes 10.0.1.2/32 path 1 community

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes <route-id> path <path-id> ext-community

Shows information about the extended communities for a specific IPv4 received route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 route.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes 10.0.1.2/32 path 1 ext-community

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes <route-id> path <path-id> flags

Shows information about flags for a specific IPv4 received route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 route.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes 10.0.1.2/32 path 1 flags
    operational
    -----------
    multipath

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes <route-id> path <path-id> large-community

Shows information about the large communities for a specific IPv4 received route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 route.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes 10.0.1.2/32 path 1 large-community

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes <route-id> path <path-id> nexthop

Shows information about the next hops for a specific IPv4 received route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 route.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes 10.0.1.2/32 path 1 nexthop

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes <route-id> path <path-id> nexthop <nexthop-id>

Shows information about a specific next hop for a specific IPv4 received route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 route.
`<path-id>` | The path ID.
`<nexthop-id>` | The nexthop ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes 10.0.1.2/32 path 1 nexthop 1

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast received-routes <route-id> path <path-id> peer

Shows information about peers for a specific IPv4 received route path ID for a BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.
`<route-id>` | The IPv4 route.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast received-routes 10.0.1.2/32 path 1 peer

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unicast route-counters

Shows the number of IPv4 routes for a specific BGP neighbor in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The IP address of the BGP neighbor or the interface if you are using unnumbered BGP.

### Version History

Introduced in Cumulus Linux 5.5.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unicast route-counters
                    operational
    --------------  -----------
    route-count     8
    adj-rib-in      0
    damped          0
    removed         0
    history         0
    stale           0
    valid           8
    all-rib         8
    routes-counted  8
    best-routes     3
    usable          8

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unreachability advertised-routes

Shows BGP unreachability advertised routes for the BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unreachability advertised-routes

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unreachability aspath

Shows BGP unreachability AS path configuration for the specified neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unreachability aspath
                     operational  applied
    ---------------  -----------  --------
    replace-peer-as  disabled     disabled
    private-as       none         none
    allow-my-asn
      state          enabled      enabled
      origin         enabled      enabled

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unreachability capabilities

Shows BGP unreachability capabilities for the specified neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unreachability capabilities

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unreachability graceful-restart

Shows BGP unreachability graceful restart timers for the specified neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unreachability graceful-restart

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family ipv4-unreachability prefix-limits

Shows BGP unreachability prefix-limits for the specified neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family ipv4-unreachability prefix-limits
                       operational  applied
    -----------------  -----------  -------
    maximum                         6
    warning-threshold               75

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> bfd

Shows BFD configuration for the specified BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.15.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 bfd
            applied
    ------  -------
    enable  off

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> capabilities

Shows the capabilities for the specified BGP neighbor, such as if extended next hop and 32-bit ASN transmission are enabled.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 capabilities
                      operational  applied
    ----------------  -----------  -------
    extended-nexthop               auto

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> ebgp-policy

Shows the Default External BGP (EBGP) route propagation behavior for the specified BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 ebgp-policy
      operational
      -----------
      inbound
      outbound
      inbound
      outbound

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> graceful-restart

Shows BGP graceful restart configuration for the specified BGP neighbor. BGP graceful restart minimizes the negative effects that occur when BGP restarts.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.1.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 graceful-restart
                     operational    applied
    ---------------  -------------  -------
    remote-mode      NotApplicable
    rx-restart-time  120
    mode                            auto

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> local-as

Shows the local AS for the specified BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 local-as
            applied
    ------  -------
    enable  off

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> message-stats

Shows message statistics for the BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.8.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 message-stats
                       operational
    ------------------  -----------
    input-queue         0
    output-queue        0
    rx-opens            1
    tx-opens            1
    rx-keepalives       848
    tx-keepalives       848
    rx-route-refreshes  0
    tx-route-refreshes  0
    tx-total            916
    rx-total            933

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> nexthop

Shows the BGP neighbor next hop.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 nexthop
                 operational
    -----------  -------------------------
    ipv4         10.10.10.1
    ipv6-global  fe80::4ab0:2dff:fed1:9b88
    ipv6-local   fe80::4ab0:2dff:fed1:9b88

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> timers

Shows timer configuration for the specified BGP neighbor, such as the reconnect, advertisement and keepalive intervals, and the hold time.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp52 timers
                         operational  applied  pending
    -------------------  -----------  -------  -------
    connection-retry     10           auto     auto
    hold                 9000         auto     auto
    keepalive            3000         auto     auto
    route-advertisement               auto     auto

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> ttl-security

Shows BGP TTL security configuration for the specified BGP neighbor. BGP TTL security prevents attacks against eBGP, such as denial of service (DoS) attacks.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 ttl-security
            operational  applied
    ------  -----------  -------
    enable  on           off
    hops    1

## nv show vrf <vrf-id> router bgp nexthop

Shows BGP next hop information for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp nexthop
    PathCnt - Number of paths pointing to this Nexthop, ResolvedVia - Resolved via
    address or interface, Interface - Resolved via interface

    Afi   Address                    IGPMetric  Valid  PathCnt  ResolvedVia                Interface
    ----  -------------------------  ---------  -----  -------  -------------------------  ---------
    ipv4  10.10.10.2                 0          on     54       fe80::4ab0:2dff:fe08:9898  swp51
                                                                fe80::4ab0:2dff:fed8:67cb  swp52
          10.10.10.3                 0          on     36       fe80::4ab0:2dff:fe08:9898  swp51
                                                                fe80::4ab0:2dff:fed8:67cb  swp52
          10.10.10.4                 0          on     36       fe80::4ab0:2dff:fe08:9898  swp51
                                                                fe80::4ab0:2dff:fed8:67cb  swp52
    ipv6  fe80::4ab0:2dff:fe08:9898  0          on     6        swp51
          fe80::4ab0:2dff:fed8:67cb  0          on     6        swp51

## nv show vrf <vrf-id> router bgp nexthop <afi>

Shows BGP next hop information for IPv4 or IPv6 for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<afi>` | The address family: IPv4 or IPv6.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp nexthop ipv4
    Nexthops
    ===========

        PathCnt - Number of paths pointing to this Nexthop, ResolvedVia - Resolved via
        address or interface, Interface - Resolved via interface

        Address     IGPMetric  Valid  PathCnt  ResolvedVia                Interface
        ----------  ---------  -----  -------  -------------------------  ---------
        10.10.10.2  0          on     54       fe80::4ab0:2dff:fe08:9898  swp51
                                               fe80::4ab0:2dff:fed8:67cb  swp52
        10.10.10.3  0          on     36       fe80::4ab0:2dff:fe08:9898  swp51
                                               fe80::4ab0:2dff:fed8:67cb  swp52
        10.10.10.4  0          on     36       fe80::4ab0:2dff:fe08:9898  swp51
                                               fe80::4ab0:2dff:fed8:67cb  swp52

## nv show vrf <vrf-id> router bgp nexthop <afi> ip-address

Shows BGP IPv4 or IPv6 next hops for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<afi>` | The address family: IPv4 or IPv6.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp nexthop ipv4 ip-address
    PathCnt - Number of paths pointing to this Nexthop, ResolvedVia - Resolved via
    address or interface, Interface - Resolved via interface

    Address     IGPMetric  Valid  PathCnt  ResolvedVia                Interface
    ----------  ---------  -----  -------  -------------------------  ---------
    10.10.10.2  0          on     54       fe80::4ab0:2dff:fe08:9898  swp51
                                                                      swp52
    10.10.10.3  0          on     36       fe80::4ab0:2dff:fe08:9898  swp51
                                                                      swp52
    10.10.10.4  0          on     36       fe80::4ab0:2dff:fe08:9898  swp51
                                                                      swp52

## nv show vrf <vrf-id> router bgp nexthop <afi> ip-address <ip-address>

Shows information about a specific BGP IPv4 or IPv6 next hop for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<afi>` | The address family: IPv4 or IPv6.
`<ip-address>` | The IPv4 or IPv6 address.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp nexthop ipv4 ip-address 10.10.10.2
                      operational
    ----------------  -------------------------
    valid             yes
    complete          on
    igp-metric        0
    path-count        15
    last-update-time  2024-11-14T08:58:31Z
    [resolved-via]    fe80::4ab0:2dff:fe5e:b1fc
    ...

## nv show vrf <vrf-id> router bgp nexthop <afi> ip-address <ip-address> path

Shows all paths associated with BGP IPv4 or IPv6 nexthops for the specified VRF.

Add `-o json` at the end of the command to see the output in a more readable format.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<afi>` | The address family: IPv4 or IPv6.
`<ip-address>` | The IPv4 or IPv6 address.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp nexthop ipv4 ip-address 10.10.10.2 path -o json
    {
      "1": {
        "address-family": "l2vpn-evpn",
        "flags": {
          "damped": "off",
          "deterministic-med-selected": "on",
          "history": "off",
          "multipath": "off",
          "nexthop-self": "off",
          "removed": "off",
          "selected": "off",
          "stale": "off",
          "valid": "on"
        },
        "flags-string": "vd",
        "prefix": "[5]:[0]:[24]:[10.1.20.0]",
        "rd": "10.10.10.2:3",
        "vrf": "default"
      },
      "2": {
        "address-family": "l2vpn-evpn",
        "flags": {
          "damped": "off",
          "deterministic-med-selected": "on",
          "history": "off",
          "multipath": "off",
          "nexthop-self": "off",
          "removed": "off",
          "selected": "off",
          "stale": "off",
          "valid": "on"
        },
        "flags-string": "vd",
        "prefix": "[5]:[0]:[24]:[10.1.10.0]",
        "rd": "10.10.10.2:3",
        "vrf": "default"
      },
      "3": {
        "address-family": "l2vpn-evpn",
        "flags": {
          "damped": "off",
          "deterministic-med-selected": "on",
          "history": "off",
          "multipath": "off",
          "nexthop-self": "off",
          "removed": "off",
          "selected": "off",
          "stale": "off",
          "valid": "on"
        },
        "flags-string": "vd",
        "prefix": "[5]:[0]:[24]:[10.1.30.0]",
        "rd": "10.10.10.2:2",
        "vrf": "default"
      },
      "4": {
        "address-family": "l2vpn-evpn",
        "flags": {
          "damped": "off",
          "deterministic-med-selected": "off",
          "history": "off",
          "multipath": "off",
          "nexthop-self": "off",
          "removed": "off",
          "selected": "off",
          "stale": "off",
          "valid": "on"
        },
        "flags-string": "v",
        "prefix": "[5]:[0]:[24]:[10.1.20.0]",
        "rd": "10.10.10.2:3",
        "vrf": "default"
      }
    ...
    }

## nv show vrf <vrf-id> router bgp nexthop <afi> ip-address <ip-address> path <path-id>

Shows information about a specific path associated with BGP IPv4 or IPv6 nexthops for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<afi>` | The address family: IPv4 or IPv6.
`<ip-address>` | The IPv4 or IPv6 address.
`<path-id>` | The path ID.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp nexthop ipv4 ip-address 10.10.10.2 path 1
                                  operational
    ----------------------------  ------------------------
    address-family                l2vpn-evpn
    prefix                        [5]:[0]:[24]:[10.1.20.0]
    rd                            10.10.10.2:3
    vrf                           default
    flags-string                  vd
    flags
      damped                      off
      history                     off
      selected                    off
      valid                       on
      deterministic-med-selected  on
      stale                       off
      removed                     off
      multipath                   off
      nexthop-self                off

## nv show vrf <vrf-id> router bgp nexthop <afi> ip-address <ip-address> resolved-via

Shows the recursive BGP IPv4 or IPv6 next hops for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<afi>` | The address family: IPv4 or IPv6.
`<ip-address>` | The IPv4 or IPv6 address.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp nexthop ipv4 ip-address 10.10.10.2 resolved-via
    Nexthop                    interface
    -------------------------  ---------
    fe80::4ab0:2dff:fe08:9898  swp51
    fe80::4ab0:2dff:fed8:67cb  swp52

## nv show vrf <vrf-id> router bgp path-selection

Shows the BGP path selection configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp path-selection
                             applied
    -----------------------  ---------
    routerid-compare         off
    aspath
      compare-lengths        on
      compare-confed         off
    med
      compare-always         off
      compare-deterministic  on
      compare-confed         off
      missing-as-max         off
    multipath
      aspath-ignore          off
      generate-asset         off
      bandwidth              all-paths

## nv show vrf <vrf-id> router bgp path-selection aspath

Shows the BGP AS path selection configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp path-selection aspath
                     applied
    ---------------  -------
    compare-lengths  on
    compare-confed   off

## nv show vrf <vrf-id> router bgp path-selection med

Shows the BGP med path selection configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp path-selection med
                           applied
    ---------------------  -------
    compare-always         off
    compare-deterministic  on
    compare-confed         off
    missing-as-max         off

## nv show vrf <vrf-id> router bgp path-selection multipath

Shows BGP multipath path selection configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp path-selection multipath
                    applied
    --------------  ---------
    aspath-ignore   off
    generate-asset  off
    bandwidth       all-paths

## nv show vrf <vrf-id> router bgp peer-group

Shows the peer groups configured for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group
    RemoteAs - Remote Autonomous System, Afi-Safi - Address family

    Name      RemoteAs  Type      Afi-Safi  MemberCount
    --------  --------  --------  --------  -----------
    underlay            external            5

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id>

Shows global configuration for the specified peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group underlay
    password                                    $nvsec$d1a028e8c7f97db92876c2a30fcc403f
    enforce-first-as                            off
    passive-mode                                off
    nexthop-connected-check                     on
    description                                 none
    bfd
      enable                                    off
    ttl-security
      enable                                    off
    local-as
      enable                                    off
    timers
      keepalive                                 auto
      hold                                      auto
      connection-retry                          auto
      route-advertisement                       auto
    address-family
      ipv4-unicast
        enable                                  on
        route-reflector-client                  off
        soft-reconfiguration                    off
        nexthop-setting                         auto
        add-path-tx                             off
        attribute-mod
          aspath                                on
          med                                   on
          nexthop                               on
        aspath
          replace-peer-as                       off
          private-as                            none
          allow-my-asn
            enable                              off
    ...

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family

Shows configuration information for the address families (IPv4, IPv6, EVPN).

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family
                                 operational  applied
    ---------------------------  -----------  -------
    ipv4-unicast
      enable                                  on
      route-reflector-client                  off
      soft-reconfiguration                    off
      nexthop-setting                         auto
      add-path-tx                             off
      attribute-mod
        aspath                                on
        med                                   on
        nexthop                               on
      aspath
        replace-peer-as                       off
        private-as                            none
        allow-my-asn
          enable                              off
      weight                                  0
      community-advertise
        regular                               on
        extended                              on
        large                                 off
      conditional-advertise
        enable                                off
      policy
        inbound
          route-map                           none
          prefix-list                         none
          aspath-list                         none
    ...

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unicast

Shows the configuration for the specified BGP IPv4 peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unicast
                               operational  applied
    -------------------------  -----------  -------
    enable                                  on
    route-reflector-client                  off
    route-server-client                     off
    soft-reconfiguration                    off
    nexthop-setting                         auto
    add-path-tx                             off
    attribute-mod
      aspath                                on
      med                                   on
      nexthop                               on
    aspath
      replace-peer-as                       off
      private-as                            none
      allow-my-asn
        enable                              off
    weight                                  0
    community-advertise
      regular                               on
      extended                              on
      large                                 off
    conditional-advertise
      enable                                off
    policy
      inbound
        route-map                           none
        prefix-list                         none
        aspath-list                         none
      outbound
        route-map                           none
        unsuppress-map                      none
        prefix-list                         none
        aspath-list                         none
    ...

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unicast aspath

Shows the configuration settings for handling the AS path for prefixes to and from the specified BGP IPv4 peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unicast aspath
                     operational  applied
    ---------------  -----------  -------
    replace-peer-as               off
    private-as                    none
    allow-my-asn
      enable                      off

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unicast aspath allow-my-asn

Shows if it is acceptable for a received AS path from the specified BGP IPv4 peer group to contain the ASN of the local system.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unicast aspath allow-my-asn
            operational  applied
    ------  -----------  -------
    enable               off

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unicast attribute-mod

Shows the attribute modification configuration settings for the specified BGP IPv4 peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unicast attribute-mod
             operational  applied
    -------  -----------  -------
    aspath                on
    med                   on
    nexthop               on

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unicast community-advertise

Shows community advertise configuration information for the specified BGP IPv4 peer group. The community advertise option determines if the neighbor can advertise a prefix to any iBGP or eBGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unicast community-advertise
              operational  applied
    --------  -----------  -------
    regular                on
    extended               on
    large                  off

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unicast conditional-advertise

Shows conditional advertisement configuration information for the specified BGP IPv4 peer group. The BGP conditional advertisement option lets you advertise certain routes only if other routes either do or do not exist.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unicast conditional-advertise
                   applied  pending
    -------------  -------  -----------
    enable         off      on
    advertise-map           myadvertise
    exist-map               EXIST
    non-exist-map           NONEXIST

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unicast default-route-origination

Shows default route origination configuration for the specified BGP IPv4 peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unicast default-route-origination
            applied
    ------  -------
    state   disabled

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unicast policy

Shows the policies configured for the specified BGP IPv4 peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unicast policy
                      applied
    ----------------  ----------
    inbound
      route-map       myroutemap-in
      aspath-list     none
      prefix-list     none
    outbound
      route-map       myroutemap-out
      unsuppress-map  none
      aspath-list     none
      prefix-list     none

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unicast policy inbound

Shows the inbound policy for the specified BGP IPv4 peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unicast policy inbound
                 applied
    -----------  ----------
    route-map    myroutemap-in
    aspath-list  none
    prefix-list  non

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unicast policy outbound

Shows the outbound policy for the specified BGP IPv4 peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unicast policy outbound
                    applied
    --------------  -------
    route-map       myroutemap-out
    unsuppress-map  none
    aspath-list     none
    prefix-list     none

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unicast prefix-limits

Shows the limits on prefixes from the specified IPv4 peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unicast prefix-limits
                         operational  applied
    -------------------  -----------  -------
    inbound
      maximum                         none
      warning-threshold               75

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unicast prefix-limits inbound

Shows the limits on inbound prefixes from the specified IPv4 peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unicast prefix-limits inbound
                       operational  applied
    -----------------  -----------  -------
    maximum                         none
    warning-threshold               75

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unreachability aspath

Shows the BGP unreachability prefix limits for the peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unreachability aspath
                     operational  applied
    ---------------  -----------  --------
    replace-peer-as  disabled     disabled
    private-as       none         none
    allow-my-asn
      state          enabled      enabled
      origin         enabled      enabled

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family ipv4-unreachability prefix-limits

Shows the the BGP unreachability prefix limits for the peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family ipv4-unreachability prefix-limits
                       operational  applied
    -----------------  -----------  -------
    maximum                         6
    warning-threshold               75

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> bfd

Shows BFD configuration for the specified BGP peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.15.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES bfd
            operational  applied
    ------  -----------  -------
    enable               off

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> capabilities

Shows the capabilities for the specified BGP peer group, such as if extended next hop and 32-bit ASN transmission are enabled.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES capabilities
                      operational  applied
    ----------------  -----------  -------
    extended-nexthop               auto

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> local-as

Shows the local AS for the specified BGP peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES local-as
            operational  applied
    ------  -----------  -------
    enable               off

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> timers

Shows BGP timer configuration for the peer group in the specified VRF, such as the conditional advertisement, connection retry, and keepalive interval, and the hold time for keepalive messages.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES timers
                         operational  applied
    -------------------  -----------  -------
    keepalive                         auto
    hold                              auto
    connection-retry                  auto
    route-advertisement               auto

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> ttl-security

Shows BGP TTL security configuration for the specified BGP peer group. BGP TTL security prevents attacks against eBGP, such as denial of service (DoS) attacks.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES ttl-security
            applied
    ------  -------
    enable  on
    hops    3

## nv show vrf <vrf-id> router bgp route-export

Shows BGP route export configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp route-export
                      operational  applied  pending
    ----------------  -----------  -------  -------
    to-evpn
      [route-target]               auto     auto

## nv show vrf <vrf-id> router bgp route-export to-evpn

Shows BGP route export to EVPN configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.8.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp route-export to-evpn
                    operational  applied
    --------------  -----------  -------
    [route-target]               auto

## nv show vrf <vrf-id> router bgp route-import

Shows BGP route import configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp route-import
                      operational  applied
    ----------------  -----------  -------------
    from-evpn
      [route-target]               10.10.10.1:20

## nv show vrf <vrf-id> router bgp route-import from-evpn

Shows BGP route import from EVPN configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp route-import from-evpn
                    operational  applied
    --------------  -----------  -------
    [route-target]               auto

## nv show vrf <vrf-id> router bgp route-reflection

Shows BGP route reflection configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp route-reflection
            operational  applied  pending
    ------  -----------  -------  -------
    enable               off      off

## nv show vrf <vrf-id> router bgp soo-source

Configures BGP PIC anycast by setting the SOO source IP address on a leaf. Fast route convergence in case of remote link failures between leaf and spine, and spine and superspine layers requires you to configure the SOO source IP address on leaf switches to advertise the SOO route.

You configure BGP PIC anycast in addition to configuring BGP prefix independent convergence (PIC). You configure PIC with the `nv set vrf <vrf-id> router bgp address-family <address-family>-unicast advertise-origin` command and the `nv set vrf default router bgp address-family <address-family>-unicast nhg-per-origin` command.

Configuring the same SOO source IP address on multiple leaf switches puts them in the same anycast group.

The SOO source IP address must be unique in the topology so that it does not conflict with the router ID or loopback IP address of any other switch.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.16.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp soo-source 10.10.10.1

## nv show vrf <vrf-id> router bgp timers

Shows BGP timer configuration for all peers in the specified VRF, such as the conditional advertisement, connection retry, and keepalive interval, and the hold time for keepalive messages.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp timers
                           operational  applied  pending
    ---------------------  -----------  -------  -------
    conditional-advertise               60       60
    connection-retry                    10       10
    hold                                9        9
    keepalive                           3        3
    route-advertisement                 none     none