# BGP EVPN

## nv show evpn vni <vni-id> bgp-info

Shows BGP information for the specified EVPN VNI.

### Command Syntax

Syntax | Description
--- | ---
`<vni-id>` | The VNI name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show evpn vni 10 bgp-info
                               operational
    -------------------------  ------------
    rd                         10.10.10.1:6
    local-vtep                 10.0.1.12
    advertise-svi-ip           off
    advertise-default-gateway  off
    in-kernel                  on
    type                       L2
    mac-vrf-soo
    [import-route-target]      65101:10
    [export-route-target]      65101:10

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn

Shows EVPN BGP configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn
            operational  applied
    ------  -----------  -------
    enable               off

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn loc-rib

Shows the EVPN local RIB for the specified VRF.

Cumulus Linux 5.11 and later no longer provides this command. Use the `nv show vrf <vrf-id> router bgp address-family l2vpn-evpn route` command instead.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn loc-rib
    rd
    =====
                  Summary
    ------------  -------------
    10.10.10.1:2  route-type: 1
                  route-type: 2
                  route-type: 3
    10.10.10.1:3  route-type: 1
                  route-type: 4
    10.10.10.1:4  route-type: 1
                  route-type: 2
                  route-type: 3
    10.10.10.1:5  route-type: 1
                  route-type: 2
                  route-type: 3
    10.10.10.1:6  route-type: 5
    10.10.10.1:7  route-type: 5
    10.10.10.1:8  route-type: 1
    ...

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn loc-rib rd

Shows the EVPN local RIB RDs for the specified VRF.

Cumulus Linux 5.11 and later no longer provides this command.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn loc-rib rd
                  Summary
    ------------  -------------
    10.10.10.1:2  route-type: 1
                  route-type: 2
                  route-type: 3
    10.10.10.1:3  route-type: 1
                  route-type: 4
    10.10.10.1:4  route-type: 1
                  route-type: 2
                  route-type: 3
    10.10.10.1:5  route-type: 1
                  route-type: 2
                  route-type: 3
    10.10.10.1:6  route-type: 5
    10.10.10.1:7  route-type: 5
    10.10.10.1:8  route-type: 1
                  route-type: 4
    ...

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn loc-rib rd <rd-id>

Shows a specific EVPN local RIB RD for the specified VRF.

Cumulus Linux 5.11 and later no longer provides this command.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<rd-id>` | The route distinguisher ID.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn loc-rib rd 10.10.10.1:9
                  operational  applied
    ------------  -----------  -------
    [route-type]  1
    [route-type]  4

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn loc-rib rd <rd-id> route-type

Shows the EVPN local RIB RD route distinguisher route types for the specified VRF.

Cumulus Linux 5.11 and later no longer provides this command.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<rd-id>` | The route distinguisher ID: `ead`, `macip`, `multicast`, `ethernet-segment`, `prefix`, or an integer between 1 and 5.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn loc-rib rd 10.10.10.1:9 route-type
      Summary
    -  ---------------------------------------------------------------------------------
    1  route: 03:44:38:39:be:ef:aa:00:00:03+::]/352+03:44:38:39:be:ef:aa:00:00:03+::/352
    4  route:                               03:44:38:39:be:ef:aa:00:00:03+10.10.10.1/352

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn loc-rib rd <rd-id> route-type <route-type-id>

Shows information about a specific EVPN local RIB RD route distinguisher route type for the specified VRF.

Cumulus Linux 5.11 and later no longer provides this command.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<rd-id>` | The route distinguisher ID.
`<route-type-id>` | The route type: `ead`, `macip`, `multicast`, `ethernet-segment`, `prefix`, or an integer between 1 and 5.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn loc-rib rd 10.10.10.1:20 route-type multicast
    route

    ========

          Advto - peers the prefix is advertised to, EVPNPrefixStr - EVPN prefix string

        (Mac + IP), MAC - MAC Address, Peer - neighbor router-id, PathCnt - number of

        L2VPN EVPN per (RD, route-type) paths

        Route      Advto  EVPNPrefixStr           MAC  Peer                PathCnt  VNI  Weight

        ---------  -----  ----------------------  ---  ------------------  -------  ---  ------

        0+1.1.1.1  swp1   [3]:[0]:[32]:[1.1.1.1]       id: 0.0.0.0         1        101  32768

                                                       router-id: 1.1.1.1

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn loc-rib rd <rd-id> route-type <route-type-id> route

Shows the routes in the EVPN local RIB for the specified VRF with a specific RD and route type.

Cumulus Linux 5.11 and later no longer provides this command.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<rd-id>` | The route distinguisher ID.
`<route-type-id>` | The route type: `ead`, `macip`, `multicast`, `ethernet-segment`, `prefix`, or an integer between 1 and 5.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn loc-rib rd 10.10.10.1:20 route-type multicast route

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn loc-rib rd <rd-id> route-type <route-type-id> route <evpn-route-id>

Shows the routes in the EVPN local RIB for the specified VRF with a specific RD route type and EVPN route type.

Cumulus Linux 5.11 and later no longer provides this command.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<rd-id>` | The route distinguisher ID.
`<route-type-id>` | The route type: `ead`, `macip`, `multicast`, `ethernet-segment`, `prefix`, or an integer between 1 and 5.
`<evpn-route-id>` | The EVPN route type.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn loc-rib rd 10.10.10.1:20 route-type multicast route

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn route

Shows BGP EVPN routing table.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.11.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn route
    PathCnt - number of L2VPN EVPN per (RD, route-type) paths

    Route                                                                   rd             route-type  PathCnt
    ----------------------------------------------------------------------  -------------  ----------  -------
    [10.10.10.1:2]:[5]:[0]:[10.1.30.0/24]                                   10.10.10.1:2   5           5
    [10.10.10.1:3]:[5]:[0]:[10.1.10.0/24]                                   10.10.10.1:3   5           5
    [10.10.10.1:3]:[5]:[0]:[10.1.20.0/24]                                   10.10.10.1:3   5           5
    [10.10.10.2:2]:[5]:[0]:[10.1.30.0/24]                                   10.10.10.2:2   5           1
    [10.10.10.2:3]:[5]:[0]:[10.1.10.0/24]                                   10.10.10.2:3   5           1
    [10.10.10.2:3]:[5]:[0]:[10.1.20.0/24]                                   10.10.10.2:3   5           1
    [10.10.10.2:4]:[2]:[0]:[44:38:39:22:01:7a]                              10.10.10.2:4   2           1
    [10.10.10.2:4]:[2]:[0]:[48:b0:2d:a4:0d:7a]                              10.10.10.2:4   2           1
    [10.10.10.2:4]:[2]:[0]:[48:b0:2d:a4:0d:7a]:[fe80::4ab0:2dff:fea4:d7a]   10.10.10.2:4   2           1
    [10.10.10.2:4]:[2]:[0]:[48:b0:2d:bc:36:08]                              10.10.10.2:4   2           1
    [10.10.10.2:4]:[3]:[0]:[10.0.1.12]                                      10.10.10.2:4   3           1
    [10.10.10.2:5]:[2]:[0]:[44:38:39:22:01:7a]                              10.10.10.2:5   2           1
    [10.10.10.2:5]:[2]:[0]:[48:b0:2d:7b:a7:e9]                              10.10.10.2:5   2           1
    [10.10.10.2:5]:[2]:[0]:[48:b0:2d:9a:8d:47]                              10.10.10.2:5   2           1
    [10.10.10.2:5]:[2]:[0]:[48:b0:2d:9a:8d:47]:[fe80::4ab0:2dff:fe9a:8d47]  10.10.10.2:5   2           1
    [10.10.10.2:5]:[3]:[0]:[10.0.1.12]                                      10.10.10.2:5   3           1
    [10.10.10.2:6]:[2]:[0]:[44:38:39:22:01:7a]                              10.10.10.2:6   2           1
    [10.10.10.2:6]:[2]:[0]:[48:b0:2d:72:90:d7]                              10.10.10.2:6   2           1
    ...

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn route <route-id>

Shows information about the BGP EVPN route.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.11.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn route 10.10.10.1:3

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn route-count

Shows the BGP EVPN route and path count.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.11.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn route-count
                  operational
    ------------  -----------
    total-routes  63
    total-paths   243

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn update-group

Shows information about BGP EVPN update group events.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn update-group
    RouteMap - Outbound route map, MinAdvInterval - Minimum route advertisement
    interval, CreationTime - Time when the update group was created, LocalAsChange -
    LocalAs changes for inbound route, Flags - r - replace-as, x - no-prepend

    UpdateGrp  RouteMap  MinAdvInterval  CreationTime          LocalAsChange  Flags
    ---------  --------  --------------  --------------------  -------------  -----
    2                    0               2024-11-14T08:58:25Z

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn update-group <group-id>

Shows information about a specific BGP EVPN update group.

In Cumulus Linux 5.10 and earlier, add `-o json` at the end of the command to see the output in a more readable format.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<group-id>` | The BGP group ID.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn update-group 2
                                      operational
    --------------------------------  --------------------
    update-group-id                   2
    min-route-advertisement-interval  0
    create-time                       2024-11-15T10:01:47Z

    sub-group
    ============

        CreateTime - Time when the sub group was created, AdvRouteCnt - Number of routes
        advertised to peer, Refresh - Indicates if subgroup requires refresh,
        TotalQueuePkt - Total packets in queue, TotalEnqueuePkt - Total packets
        enqueued, PktQueueLength - Packet queue length, Neighbor - Sub group peer info

        GrpID  CreateTime            AdvRouteCnt  Refresh  TotalQueuePkt  TotalEnqueuePkt  PktQueueLength  Neighbor
        -----  --------------------  -----------  -------  -------------  ---------------  --------------  -------------
        2      2024-11-15T10:01:47Z  72           off      104            104              0               peerlink.4094
                                                                                                           swp52
                                                                                                           swp53
                                                                                                           swp54

## nv show vrf <vrf-id> router bgp address-family l2vpn-evpn update-group <group-id> sub-group

Shows the subgroup information for a specific BGP EVPN update group.

In Cumulus Linux 5.10 and earlier, add `-o json` at the end of the command to see the output in a more readable format.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<group-id>` | The BGP group ID.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp address-family l2vpn-evpn update-group 2 sub-group

    CreateTime - Time when the sub group was created, AdvRouteCnt - Number of routes
    advertised to peer, Refresh - Indicates if subgroup requires refresh,
    TotalQueuePkt - Total packets in queue, TotalEnqueuePkt - Total packets
    enqueued, PktQueueLength - Packet queue length, Neighbor - Sub group peer info

    GrpID  CreateTime            AdvRouteCnt  Refresh  TotalQueuePkt  TotalEnqueuePkt  PktQueueLength  Neighbor
    -----  --------------------  -----------  -------  -------------  ---------------  --------------  -------------
    2      2024-11-15T10:01:47Z  72           off      104            104              0               peerlink.4094
                                                                                                       swp52
                                                                                                       swp53
                                                                                                       swp54

## nv show vrf <vrf-id> evpn bgp-info

Shows layer 3 VNI information from BGP for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.4.0

### Example

    cumulus@switch:~$ nv show vrf RED evpn bgp-info
                           operational
    ---------------------  -----------------
    rd                     10.10.10.1:3
    local-vtep             10.0.1.12
    router-mac             44:38:39:be:ef:aa
    system-mac             44:38:39:22:01:7a
    system-ip              10.10.10.1
    [import-route-target]  65101:4001
    [export-route-target]  65101:4001

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn

Shows EVPN configuration for the specified BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family l2vpn-evpn
                           operational  applied
    ---------------------  -----------  -------
    enable                              on
    attribute-mod
      aspath               off
      med                  off
      nexthop              on
    graceful-restart
      rx-eof-rib           off
      tx-eof-rib           off
    prefix-limits
      inbound
        maximum            1
        warning-threshold  75
        warning-only       off

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn attribute-mod

Shows the attribute modification configuration settings for the specified neighbor for EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family l2vpn-evpn attribute-mod
             operational  applied
    -------  -----------  -------
    aspath   off
    med      off
    nexthop  on

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn aspath

Shows the configuration options for handling the AS path for prefixes to and from the specified BGP neighbor for EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family l2vpn-evpn aspath

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn aspath allow-my-asn

Shows if it is acceptable for a received AS path to contain the ASN of the local system for EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family l2vpn-evpn aspath allow-my-asn

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn graceful-restart

Shows graceful restart configuration for the specified BGP neighbor for EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family l2vpn-evpn graceful-restart
                operational
    ----------  -----------
    rx-eof-rib  on
    tx-eof-rib  on

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn graceful-restart timers

Shows the BGP graceful restart selection deferral and stale path timer settings for the specified neighbor for EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.9.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family l2vpn-evpn graceful-restart timers

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn graceful-restart timers stale-path

Shows the BGP graceful restart stale path timer settings for the specified neighbor for EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.9.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family l2vpn-evpn graceful-restart timers stale-path

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn graceful-restart timers selection-deferral

Shows the BGP graceful restart selection deferral timer for the specified neighbor for EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.9.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family l2vpn-evpn graceful-restart timers selection-deferral

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn policy

Shows EVPN policies for the specified neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family l2vpn-evpn policy
                      operational  applied
    ----------------  -----------  -------
    inbound
      route-map       MAP1         MAP1
    outbound
      route-map                    none
      unsuppress-map               none

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn policy inbound

Shows the inbound EVPN policy for the specified BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family l2vpn-evpn policy inbound
               operational  applied
    ---------  -----------  -------
    route-map  MAP1         MAP1

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn policy outbound

Shows the outbound EVPN policy for the specified BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family l2vpn-evpn policy outbound
                    operational  applied
    --------------  -----------  -------
    route-map                    none
    unsuppress-map               none

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn capabilities

Shows all advertised and received EVPN capabilities for the specified BGP neighbor.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp neighbor swp51 address-family l2vpn-evpn capabilities
                         operational
    -------------------  -----------
    rx-addpath           on
    rx-graceful-restart  on
    rx-mpbgp             on
    tx-addpath           off
    tx-mpbgp             on

## nv show vrf <vrf-id> router bgp neighbor <neighbor-id> address-family l2vpn-evpn prefix-limits inbound

Shows the configured prefix limits from the specified neighbor for EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<neighbor-id>` | The BGP neighbor name or interface (for BGP unnumbered).

### Version History

Introduced in Cumulus Linux 5.10.0

### Example

    cumulus@switch:~$ nv show  vrf default router bgp neighbor swp51 address-family l2vpn-evpn prefix-limits inbound
                       operational  applied
    -----------------  -----------  -------
    maximum                         none
    warning-threshold               75
    warning-only       off

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family l2vpn-evpn

Shows configuration information for the specified BGP peer group for EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family l2vpn-evpn
            applied
    ------  -------
    enable  off

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family l2vpn-evpn attribute-mod

Shows the attribute modification configuration settings for the specified BGP peer group for EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family l2vpn-evpn attribute-mod

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family l2vpn-evpn aspath

Shows the configuration settings for handling the AS path for prefixes to and from the specified BGP peer group for EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family l2vpn-evpn aspath

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family l2vpn-evpn aspath allow-my-asn

Shows if it is acceptable for a received AS path from the specified BGP peer group to contain the ASN of the local system for EVPN.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family l2vpn-evpn aspath allow-my-asn

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family l2vpn-evpn policy

Shows the EVPN policies for the specified BGP peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family l2vpn-evpn policy

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family l2vpn-evpn policy inbound

Shows the inbound EVPN policy for the specified BGP peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family l2vpn-evpn policy inbound

## nv show vrf <vrf-id> router bgp peer-group <peer-group-id> address-family l2vpn-evpn policy outbound

Shows the outbound EVPN policy for the specified BGP peer group.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<peer-group-id>` | The peer group name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp peer-group SPINES address-family l2vpn-evpn policy outbound

## nv show vrf <vrf-id> router bgp route-export

Shows BGP route export configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp route-export
                      operational  applied  pending
    ----------------  -----------  -------  -------
    to-evpn
      [route-target]               auto     auto

## nv show vrf <vrf-id> router bgp route-export to-evpn

Shows BGP route export to EVPN configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp route-export to-evpn route-target

## nv show vrf <vrf-id> router bgp route-export to-evpn route-target

Shows the RTs configured for BGP route export for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp route-export to-evpn route-target

## nv show vrf <vrf-id> router bgp route-export to-evpn route-target <rt-id>

Shows BGP route export configuration for a specific RT in the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<rt-id>` | The route target.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp route-export to-evpn route-target 10.10.10.1:20

## nv show vrf <vrf-id> router bgp route-import from-evpn

Shows BGP route import from EVPN configuration for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp route-import from-evpn route-target

## nv show vrf <vrf-id> router bgp route-import from-evpn route-target

Shows the RTs configured for BGP route import from EVPN for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp route-import from-evpn route-target

## nv show vrf <vrf-id> router bgp route-import from-evpn route-target <rt-id>

Shows configuration for a specific RD and layer 3 RT for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<rt-id>` | The route target.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router bgp route-import from-evpn route-target 10.10.10.1:20