# RADIUS

## nv show system aaa radius

Shows the RADIUS configuration settings.

Cumulus Linux 5.12 and later no longer shows the `enable` setting; the `nv set system aaa radius enable` command is no longer provided.

### Version History

Introduced in Cumulus Linux 5.7.0

### Example

    cumulus@switch:~$ nv show system aaa radius
                     operational    applied
    ---------------  -------------  -------------
    enable           on             on
    vrf              mgmt           mgmt
    debug            enabled        enabled
    privilege-level  10             10
    retransmit       8              8
    port                            1812
    timeout                         10
    source-ipv4                     192.168.1.10
    [server]         192.168.0.254  192.168.0.254

## nv show system aaa radius server

Shows a list of the RADIUS servers configured on the switch and their configuration settings.

### Version History

Introduced in Cumulus Linux 5.7.0

### Example

    cumulus@switch:~$ nv show system aaa radius server
    Hostname       Port  Priority  Password  source-ip     Timeout
    -------------  ----  --------  --------  ------------  -------
    192.168.0.254  42    1         *         192.168.1.10  10

## nv show system aaa radius server <hostname-id>

Shows configuration settings for a specific RADIUS server.

### Command Syntax

Syntax | Description
--- | ---
`<hostname-id>` | The IP address or hostname of the RADIUS server.

### Version History

Introduced in Cumulus Linux 5.7.0

### Example

    cumulus@switch:~$ nv show system aaa radius server 192.168.0.254
               operational   applied
    ---------  ------------  ------------
    port       42            42
    timeout    10            10
    secret     *             *
    priority   1             10
    source-ip  192.168.1.10  192.168.1.10