# Static Routing

## nv show vrf <vrf-id> router static <route-id>

Shows configuration information about the static route for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IP prefix.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router static 10.10.10.101/32
                    applied
    --------------  ------------
    tag             none
    [via]           10.10.10.1
    address-family  ipv4-unicast
    [distance]      2

## nv show vrf <vrf-id> router static <route-id> distance <distance-id>

Shows information about the administrative distance for the static route for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IP prefix.
`<distance-id>` | The path distance.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router static 10.10.10.101/32 distance 2
          applied
    -----  ----------
    tag    none
    [via]  10.0.1.0
    [via]  10.10.10.1

## nv show vrf <vrf-id> router static <route-id> distance <distance-id> via <via-id>

Shows information about the administrative distance for the static route and next hop for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IP prefix.
`<distance-id>` | The path distance.
`<via-id>` | The IP address, interface, or `blackhole`.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router static 10.10.10.101/32 distance 2 via 10.10.10.1
               applied
    ---------  ------------
    interface  auto
    vrf        RED
    type       ipv4-address

## nv show vrf <vrf-id> router static <route-id> distance <distance-id> via <via-id> flag

Shows the flag value for the static route with a specific route prefix and distance for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IP prefix.
`<distance-id>` | The path distance.
`<via-id>` | The IP address, interface, or `blackhole`.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router static 10.10.10.101/32 distance 2 via 10.10.10.1 flag

## nv show vrf <vrf-id> router static <route-id> via <via-id>

Shows information about the next hop for the static route for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IP prefix.
`<via-id>` | The IP address, interface, or `blackhole`.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router static 10.10.10.101/32 via 10.10.10.1
               applied
    ---------  ------------
    interface  swp1
    vrf        auto
    type       ipv4-address

## nv show vrf <vrf-id> router static <route-id> via <via-id> flag

Shows the flag value for the static route with the next hop for the specified VRF.

### Command Syntax

Syntax | Description
--- | ---
`<vrf-id>` | The VRF name.
`<route-id>` | The IP prefix.
`<via-id>` | The IP address, interface, or `blackhole`.

### Version History

Introduced in Cumulus Linux 5.0.0

### Example

    cumulus@switch:~$ nv show vrf default router static 10.10.10.101/32 via 10.10.10.1 flag
    applied
      -------
      onlink