# Adaptive Routing

## nv show interface <interface-id> router adaptive-routing

Shows adaptive routing configuration settings on a specific interface.

### Command Syntax

Syntax | Description
--- | ---
`<interface-id>` | The interface name.

### Version History

Introduced in Cumulus Linux 5.1.0

### Example

    cumulus@switch:~$ nv show interface swp1 router adaptive-routing
                                applied
    --------------------------  -------
    enable                      on
    link-utilization-threshold  70

## nv show router adaptive-routing

Shows if adaptive routing is enabled on the switch.

Cumulus Linux 5.6 supports adaptive routing on Spectrum-4. Cumulus Linux 5.5 and earlier supports adaptive routing on Spectrum-3 and Spectrum-2 as a beta feature for evaluation.

### Version History

Introduced in Cumulus Linux 5.1.0

### Example

    cumulus@switch:~$ nv show router adaptive-routing
            applied
    ------  -------
    enable  on